;
; Windows XP/Server 2003/2008/Vista/7/8/2012 , PRINTER DRIVER SETUP INFORMATION FILE
;                                      Copyright(C) 2005-2013 RICOH CO.,LTD.
;

[Version]
Signature="$Windows NT$"
Class=Printer
ClassGUID={4D36E979-E325-11CE-BFC1-08002BE10318}
Provider=%M1%
CatalogFile=GNEX_GDIM.CAT
DriverVer=02/22/2013,1.0.1.0

;
; Manufacturer section.
;
; This section lists all of the manufacturers
; that we will display in the Dialog box
;
[Manufacturer]
%M1%=PrinterList_RICOH
%M2%=PrinterList_SP

[PrinterPackageInstallation]
PackageAware=TRUE

;
; Model sections.
;
; Each section here corresponds with an entry listed in the
; [Manufacturer] section, above. The models will be displayed in the order
; that they appear in the INF file.
;

[PrinterList_RICOH]
%Printer1_RICOH% = IMG_RAW1_RICOH,USBPRINT\RICOH_SP_200SF_PC_FAD92B
%Printer2_RICOH% = IMG_RAW2_RICOH,USBPRINT\RICOH_SP_201SF_PC_FADC01
%Printer3_RICOH% = IMG_RAW3_RICOH,USBPRINT\RICOH_SP_202SF_PC_FA1352

[PrinterList_SP]
%Printer1_SP% = IMG_RAW1_SP,USBPRINT\SP_200SF_PC_FAX5605
%Printer2_SP% = IMG_RAW2_SP,USBPRINT\SP_201SF_PC_FAX9354
%Printer3_SP% = IMG_RAW3_SP,USBPRINT\SP_202SF_PC_FAX9CA4

;
; Installer Sections
;
; These sections control file installation, and reference all files that
; need to be copied. The section name will be assumed to be the driver
; file, unless there is an explicit DriverFile section listed.
;

[IMG_RAW1_RICOH]
CopyFiles=IMG_FILES,UTL1_RICOH,IMG_PP_FILES,IMG_RAW_FILES,LANGMON_FILES
PrintProcessor="GNEX_IPPR,GNEX_IPPR.dll"
LanguageMonitor="GNEX PJL Monitor,GNEX_LMON.dll"
DataSection=IMG_RAW_DATA
DataFile=GNEX_GDIMAFHUcfg.xml

[IMG_RAW2_RICOH]
CopyFiles=IMG_FILES,UTL2_RICOH,IMG_PP_FILES,IMG_RAW_FILES,LANGMON_FILES
PrintProcessor="GNEX_IPPR,GNEX_IPPR.dll"
LanguageMonitor="GNEX PJL Monitor,GNEX_LMON.dll"
DataSection=IMG_RAW_DATA
DataFile=GNEX_GDIMAFHcfg.xml

[IMG_RAW3_RICOH]
CopyFiles=IMG_FILES,UTL3_RICOH,IMG_PP_FILES,IMG_RAW_FILES,LANGMON_FILES
PrintProcessor="GNEX_IPPR,GNEX_IPPR.dll"
LanguageMonitor="GNEX PJL Monitor,GNEX_LMON.dll"
DataSection=IMG_RAW_DATA
DataFile=GNEX_GDIMAFHNcfg.xml

[IMG_RAW1_SP]
CopyFiles=IMG_FILES,UTL1_SP,IMG_PP_FILES,IMG_RAW_FILES,LANGMON_FILES
PrintProcessor="GNEX_IPPR,GNEX_IPPR.dll"
LanguageMonitor="GNEX PJL Monitor,GNEX_LMON.dll"
DataSection=IMG_RAW_DATA
DataFile=GNEX_GDIMAFHUSPcfg.xml

[IMG_RAW2_SP]
CopyFiles=IMG_FILES,UTL2_SP,IMG_PP_FILES,IMG_RAW_FILES,LANGMON_FILES
PrintProcessor="GNEX_IPPR,GNEX_IPPR.dll"
LanguageMonitor="GNEX PJL Monitor,GNEX_LMON.dll"
DataSection=IMG_RAW_DATA
DataFile=GNEX_GDIMAFHSPcfg.xml

[IMG_RAW3_SP]
CopyFiles=IMG_FILES,UTL3_SP,IMG_PP_FILES,IMG_RAW_FILES,LANGMON_FILES
PrintProcessor="GNEX_IPPR,GNEX_IPPR.dll"
LanguageMonitor="GNEX PJL Monitor,GNEX_LMON.dll"
DataSection=IMG_RAW_DATA
DataFile=GNEX_GDIMAFHNSPcfg.xml


; Copy Sections
;
; Lists of files that are actually copied. These sections are referenced
; from the installer sections, above. Only create a section if it contains
; two or more files (if we only copy a single file, identify it in the
; installer section, using the @filename notation) or if it's a color
; profile (since the DestinationDirs can only handle sections, and not
; individual files).
;

[IMG_FILES]
GNEX_IGFX.dll,,,0x0000002a
GNEX_IUI.dll,,,0x0000002a
GNEX_IIME.dll,,,0x0000002a
GNEX_IENUS.dll,,,0x0000002a
GNEX_LAN-Fax_EN.chm,,,0x0000002a
GNEX_IPPR.dll,,,0x0000002a
GNEX_REC.dll,,,0x0000002a
GNEX_CP.exe,,,0x0000002a
GNEX_BMFPCFAX.dll,,,0x0000002a
GNEX_BMFBOOK.exe,,,0x0000002a

[UTL1_RICOH]
GNEX_GDIMAFHUcfg.xml,,,0x0000002a

[UTL2_RICOH]
GNEX_GDIMAFHcfg.xml,,,0x0000002a

[UTL3_RICOH]
GNEX_GDIMAFHNcfg.xml,,,0x0000002a

[UTL1_SP]
GNEX_GDIMAFHUSPcfg.xml,,,0x0000002a

[UTL2_SP]
GNEX_GDIMAFHSPcfg.xml,,,0x0000002a

[UTL3_SP]
GNEX_GDIMAFHNSPcfg.xml,,,0x0000002a


[IMG_PP_FILES]
GNEX_IPPR.dll,,,0x0000002a

[IMG_RAW_FILES]
GNEX_IO.dll
GNEX_GDIM.ini
GNEX_CP.ini

;
; Data Sections
;
; These sections contain data that is shared between devices.
;

[IMG_RAW_DATA]
DriverFile=GNEX_IGFX.dll
ConfigFile=GNEX_IUI.dll
HelpFile=%HELPFILE%


;
; Call SetupSetDirectoryId with 66000 to set the target directory at runtime
; (depending on which environment drivers are getting installed)
;

[DestinationDirs]
DefaultDestDir=66000
IMG_PP_FILES=66001
LANGMON_FILES=66002

;
;  Source Disk Section
;

[SourceDisksNames]
1 = %DISK%,,,.

[SourceDisksFiles]
GNEX_IGFX.dll   = 1
GNEX_IUI.dll    = 1
GNEX_IIME.dll   = 1
GNEX_IO.dll     = 1
GNEX_GDIMAFHUcfg.xml= 1
GNEX_GDIMAFHcfg.xml= 1
GNEX_GDIMAFHNcfg.xml= 1
GNEX_GDIMAFHUSPcfg.xml= 1
GNEX_GDIMAFHSPcfg.xml= 1
GNEX_GDIMAFHNSPcfg.xml= 1
GNEX_GDIM.ini   = 1
GNEX_CP.ini     = 1
GNEX_IENUS.dll  = 1
GNEX_LAN-Fax_EN.chm= 1
GNEX_IPPR.dll   = 1
GNEX_LMON.dll   = 1
GNEX_REC.dll    = 1
GNEX_CP.exe     = 1
GNEX_BMFPCFAX.dll   = 1
GNEX_BMFBOOK.exe    = 1

[LANGMON_FILES]
GNEX_LMON.dll,,,0x0000002a

;
; Localizable Strings
;
[Strings]
M1="RICOH"
M2="SP"
Printer1_RICOH="RICOH SP 200SF PC FAX"
Printer2_RICOH="RICOH SP 201SF PC FAX"
Printer3_RICOH="RICOH SP 202SF PC FAX"
Printer1_SP="SP 200SF PC FAX"
Printer2_SP="SP 201SF PC FAX"
Printer3_SP="SP 202SF PC FAX"
DISK="SP 200 Series PCFAX"
HELPFILE="GNEX_LAN-Fax_EN.chm"

