this manual lists all the available switches under the -ac3enc( ) section of BeSweet v1.5.
beware : switches are case-sensitive.



-b
---

Default: 384

This sets the bitrate of AC3 output.


-6ch
---
Encode a 5.1 AC3 Stream.