The files have been decompressed to your "C:\WMD20100915ia.WHQL" directory.

To install the driver, run the "INSTALL.BAT" file. If the driver installs
successfully, it will display "Installation successful."


NOTE: The driver will install only on Windows 2003 Server and Windows 2008 Server, both 32-bit and 64-bit
versions. The drivers will not become active until the machine has rebooted.

Release Notes
This driver (build 1980) includes the following changes:

1. Corrected an issue with Windows Server SQL. The way the memory is
   allocated is done in a different way for non-bus mastering driver.
2. Corrected an issue with multiple client connected to the server. 
3. Driver responsiveness was increased through optimizations.
4. 16 and 24 Bpp BSOD bug fixed
5. Fixed write combining issue
6. Fixed 1440 x 900 corruption issue
7. Added support for 1440 x 900, 1680 x 1050 and 1920 x 1200 standard timings.
8. Frame buffer shadow optimizations were enabled for pilot 2 devices and higher.

KNOWN ISSUES
------------


HISTORY
-------

Rev. 2.00.008
  - Frame buffer shadow optimizations were enabled for pilot 2 devices and higher.

Rev. 2.00.007
  - Added support for 1440 x 900, 1680 x 1050 and 1920 x 1200 standard timings.

Rev. 2.00.006
  - Fixed 1440 x 900 corruption issue

Rev. 2.00.005
  - Fixed write combining issue

Rev. 2.00.004
  - Added BugCheck module
  - Added Driver Logging module
  - Disabled frame buffer shadow optimizations for Pilot 1 products
  - Fixed write combining issue

Rev. 2.00.003
  - Added "User.EnableShadowOptimizations" registry key switch.
  - Further optimized the driver.

Rev. 2.00.002
  - 16 and 24 Bpp BSOD bug fixed

Rev. 2.00.001
  - First draft of the optimized driver

Copyright (c)2010, Emulex Corporation. All rights reserved.
