[AL-C8600]
EPWVER="3.01"
DRVNAME="EPSON AL-C8600 Advanced"
MaxCaset=3
MaxIC=2
MaxIF=2
MaxLight=1
PaperNearEnd=19
Messagetype=1
SoundNotifyEnable=0
TrayIconEnable=0
TrayIconSelected=0
TrayIconEndTime=10000
ITEMNUM=6
ITEM004=1
ITEM007=0
ITEM011=1
ITEM012=1
ITEM013=0
ITEM014=0
TIMEOUT=60
MonitorInitTime=1000
TimeOutCountConfirmErr=3
TimeOutCount=10
TimeOutCountReadyErr=1
EnableGetStatusErr=1
JobControl=2

[Language]
English=9h

[English]
RESDLL="E_L1E042.DLL"
HELPFILE="E_SMSTE2.HLP"
SHORTCUT="EPSON Status Monitor 3 Environment Check(2)"
SOUND=0
TSS001=0
TSS002=0
TSS003=0
TSS004=0
TSS005=0
TSS006=0
TSS007=0
TSS008=0
TSS009=0
TSS010=0

[Install]
REGPATH=REG1,"HKEY_LOCAL_MACHINE\Software\EPSON\STM3\Driver\EPSON AL-C8600 Advanced"
REGENTER=REG1,"InstallPath",DRIVERDIR
REGENTER=REG1,"ModelID","AL-C8600"
REGENTER=REG1,"E_SRUN",DRIVERDIR+"\E_L19042.EXE"
REGENTER=REG1,"E_SENV",DRIVERDIR+"\E_L19042.EXE"
REGENTER=REG1,"E_SICN",DRIVERDIR+"\E_L10IC2.EXE"
REGENTER=REG1,"E_STMS",DRIVERDIR+"\E_L19042.EXE"
REGENTER=REG1,"E_SRCV",DRIVERDIR+"\E_SRCV02.EXE"
REGENTER=REG1,"DepExe",DRIVERDIR+"\E_L18042.EXE"
REGENTER=REG1,"SHORTCUTEXE_R","E_SRCV02.EXE"
REGENTER=REG1,"LocalMonitoringTimer","10"
REGENTER=REG1,"NetworkMonitoringTimer","30"
REGENTER=REG1,"JobTimer","30,30,20,20:10,10,10,10"

REGENTER=REG1,"EBAPI16","EBAPI16.DLL"
REGENTER=REG1,"EBAPI32","EBAPI.DLL"

REGPATH=REG2,"HKEY_LOCAL_MACHINE\Software\EPSON\STM3\Profile"
REGENTER=REG2,"AL-C8600",DRIVERDIR+"\E_L1X042.DAT"

REGPATH=REG3,"HKEY_LOCAL_MACHINE\Software\EPSON\STM3\STMCommon"
REGENTER=REG3,"EBAPIRECOVER",1

DRVNAME="EPSON AL-C8600 Advanced"

LANGUAGEMON1="E_SLM361.DLL","EPSON V3 Monitor361"
LANGUAGEMON2="",""
LANGUAGEMON3="E_SL2361.DLL","EPSON V3 2KMonitor361"
SDKFILENAME2="EB_SET04.EXE"
ADDEEBPARAM="/TS"

SETLPT=ALL    ,"LPT_Channel00"          ,REG_DWORD,268500994
SETLPT=ALL    ,"LPT_ChnlMode00"         ,REG_DWORD,7
SETLPT=ALL    ,"LPT_Channel01"          ,REG_DWORD,268500996
SETLPT=ALL    ,"LPT_ChnlMode01"         ,REG_DWORD,3
SETLPT=ALL    ,"LPT_WriteTotalTimeOut"  ,REG_DWORD,3000
SETLPT=WIN9X  ,"LPT_ReadTotalTimeOut"   ,REG_DWORD,1000
SETLPT=WINNT40,"LPT_ReadTotalTimeOut"   ,REG_DWORD,10000
SETLPT=WIN2000,"LPT_ReadTotalTimeOut"   ,REG_DWORD,10000
SETLPT=ALL    ,"LPT_ReadIntervalTimeOut",REG_DWORD,20
SETLPT=ALL    ,"LPT_PrtMDLName"         ,REG_SZ   ,"AL-C8600"
SETLPT=ALL    ,"LPT_SetTimeOutFlag"     ,REG_DWORD,1
SETLPT=ALL    ,"LPT_StatusLength"       ,REG_DWORD,121
SETLPT=ALL    ,"LPT_DeviceIDReply"	,REG_DWORD,1
;

