## Cordless Joyboard On-Line Help

Overview • System Requirement • Installation • Uninstallation • Setting Menu • Configuration • Display Setting

### Overview

> Congratulations on your purchase of Cordless Joyboard 805 keyboard. This Cordless Joyboard 805 keyboard combines a standard keyboard layout Hot Keys. With these easy-to-use Hot Keys, you can fully maximize use of your Cordless Joyboard 805 keyboard.

### System Requirements

- Pentium processor-based PC

- MicrosoftÒ WindowsÒ 98,ME,2000, and XP

- 16 MB of RAM

- 10MB available hard-drive space

- CD-ROM drive (for installation)

- The System supporting ACPI or APMII

- ATX mother board and ATX power supply.

### Installation

> Please follow the instructions below on how to install Cordless Joyboard 805 keyboard software to your PC system.

> 1. Please insert the CD included in your package, into your CD-ROM drive.

> 2. The system will automatically run the setup.exe once after the CD is inserted. However, if the system fails to perform this procedure,

> simply double-click on the setup.exe to continue the installation procedure.

> 3. Follow all the on-screen instructions.

> Once the software installation for Cordless Joyboard 805 keyboard is completed, the icon is shown on the WindowsÒ taskbar.

> Then you can start to enjoy your Cordless Joyboard 805 keyboard.

### Uninstallation

> From the Windows Start Menu, locate uninstall under Program Files\MagicKey, and click on Uninstall Magickey program to uninstall the driver.

### Setting Menu

> Click on the Cordless Joyboard 805 keyboard icon on the taskbar will pop up the setting menu.

> 1. Options | Open the configuration dialog box and allow you to re-program the hot key function. (How to configure)
> 2. Battery Status | Display keyboard and mouse battery status.
> 3. Help | This option is to launch the on-line help which will help you to use Cordless Joyboard 805 keyboard well.
> 4. About | This option is to show the information about the Cordless Joyboard 805 keyboard driver.
> 5. Exit | This option is to close Multimedia Keyboard driver and remove it from your computer memory. If you want to reload Cordless Joyboard 805 keyboard driver, please use Windows Explorer and double click the file "c:\Program Files\MagicKey" or restart your system to run it.

> ### Configuration

> ### Internet Function

> Item | Function | Description
> 1 |  | Shortcut. Programmable hotkey.
> 2 |  | Default search website.
> 3 |  | Favorite folder.
> 4 |  | World Wide Web.
> 5 |  | Default email application.

> Multimedia Function

> Item | Function | Description
> 6 |  | Mute
> 7 |  | Previous Track
> 8 |  | Stop
> 9 |  | Play
> 10 |  | Next Track
> 11 |  | Volume Up and Volume Down

> ACPI Function

> Item | Function | Description
> 12 |  | Sleep/ Wake up

> Enhanced Function

> | Function | Description
> A |  | Function lock: Enhanced function keys for F1 to F12. Enables key functions between commands on the side of keys, and commands on the top of keys. When ¡§Fn Lock is¡¨ on, the commands on the top of keys will be enabled.
> B |  | Help: Open the ¡§Help¡¨ function for the active window.
> C |  | Undo: Cancel the previous function
> D |  | Redo: Cancel the previous undo action
> E |  | New: Create a new document or file
> F |  | Open: Open a document or file
> G |  | Close: Close a document or file at in active window
> H |  | Reply: Reply to the email in the active window.
> I |  | Fwd: Forward the email in the active window
> J |  | Send: Send the email in the active window
> K |  | Check: Check the spellings in the active window
> L |  | Save: Save the document or file in the active window
> M |  | Print: Print the document contents in the active window
> N |  | Scroll Lock: Enables arrow keys (Up, Down) to the ¡§Page up¡¨, ¡§Page Down¡¨ function by pushing the ¡§Scroll Lock¡¨ button.

> ### How to configure the programmable hotkey :

> In the options dialog box, there are 3 ways to create your own hot key functions including : Preset Function, Shortcut and Macro. Easily choose the way and the function you want to use please refer to the following steps.

> 1. Select Function Key: Please select one "Function Key" which you want to re-program the hotkey function. There are five hotkeys in this drop-down list, P1(#1),P2(#2),P3(#3),P4(#4) and P5(#5).

> 2. Preset Function : The Cordless Joyboard 805 keyboard provides 21 functions. You can easily re-program the hotkey function from choosing one from this function list.

> 3. Shortcut : This function provides you to define personal access to another application or document. By clicking the browse button , then you can select an execution file to be launched by hotkey.

> 4. Macro : `Macro can be used to enter commonly used words, lines of text or symbols with a single press of a key.`

> `Press Apply to confirm a new function for that hotkey and continue to define other functions for other hotkeys.`

> `Press OK to exit this Function Setting dialog and save all changes.`

> `Press Load Default Setting to re-load default function settings for hotkeys.`

> ### `Display Setting`

> `Caps Lock, Num Lock, Scroll Lock Status`

> Turn on/off Caps Lock, Num Lock, Scroll Lock icon on the Windows taskbar.

> `On Screen Status Display Settings`

> `The On-Screen Status Display (OSD) informs you of what function is being performed when a hotkey or On-Screen KB button is pressed. This is only displayed when a hotkey has been pressed. It appears at the left bottom of the screen for 0.5 second default timeout.`

> `1.Enable On Screen Status Display`

> `Select Enable\Disable show OSD on Monitor.`

> 2. Status Display Timeout:

> `The default display timeout is 0.5 second. However, you can change it from 0.5 second to 5 seconds.`

> 3. Test

> `The Test button can be used to view the OSD before changes are made.
> `

IBM, PC/AT and PS/2 are registered trademarks of International Business Machines Corporation.
Microsoft and Windows are registered trademarks of Microsoft Corporation in the United States of America and/or other countries.
All other trademarks are trademarks of their respective holders.