Back to Contents

# Adapter Specifications

- Intel® Centrino® Advanced-N + WiMAX 6250
- Intel® WiMAX/WiFi Link 5350
- Intel® WiMAX/WiFi Link 5150

## Intel® Centrino® Advanced-N + WiMAX 6250

Form Factor | PCI Express* Full-Mini Card and Half-Mini Card
Dimensions | Full-Mini Card: Width 2.00 in x Length 1.18 in x Height 0.18 in (50.95 mm x 30 mm x 4.5 mm) Half-Mini Card: Width 1.049 in x Length 1.18 in x Height 0.18 in (26.64 mm x 30 mm x 4.5 mm)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
Connector Interface | 52-pin Mini Card edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 95% non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 5 GHz (802.11a/n) | 2.4 GHz (802.11b/g/n)
Frequency band | 5.15 GHz - 5.85 GHz (dependent on country) | 2.400 - 2.4835 GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5 GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | 4 to 12 (dependent on country) | Channel 1-11 (US only) Channel 1-13 (Japan, Europe)
IEEE 802.11n Data Rates | Tx/Rx: 300, 270, 243, 240, 180, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2 Mbps
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
General
Operating Systems | Microsoft Windows* XP (32-bit and 64-bit) Windows Vista* (32-bit and 64-bit) Windows* 7 (32-bit and 64-bit)
Wi-Fi Alliance* certification | Wi-Fi* certification for 802.11b, 802.11g, 802.11a, 802.11h, 802.11d, WPA-Personal, WPA-Enterprise, WPA2-Personal, WPA2-Enterprise, WMM, WMM Power Save, EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
WLAN Standard | IEEE 802.11g, 802.11b, 802.11a, 802.11n
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, AES-CCMP 128-bit, WEP 128-bit and 64-bit; 802.1X: EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Product Safety | UL, C-UL, CB (IEC 60590)
WiMAX
Frequency band | 2.5-2.7 GHz (3A Profile)
Modulation | UL - QPSK, 16 QAM DL - QPSK, 16 QAM, 64 QAM
Wireless Medium | Duplex mode: TDD operations | Scalable OFDMA (SOFDMA): 512 and 1024 FFT
sub-carrier permutation: PUSC | Channel bandwidths: 5 MHz and 10 MHz
WiMAX Network Release Feature set | SPWG/NWG Release 1.0 SPWG/NWG Release 1.5
Rate Performance | 10 Mbps DL and 4 Mbps UL @ peak rate (OTA performance, 10MHz channel)
RF Transmitter Output Power | Compliance with Power class 2
WiMAX General
Operating Systems | Microsoft Windows* XP (32-bit and 64-bit) Windows Vista* (32-bit and 64-bit) Windows* 7 (32-bit and 64-bit)
Standard Compliance | 802.16e-2005 Corrigenda 2 (D4)
WiMAX System Profile Feature set | Mobile WiMAX release 1, Wave II Profile 3A
Security | Key Management Protocol (PKMv2)
Encryption | 128-bit CCMP (Counter-Mode/CBC-MAC) based on AES encryption

## Intel® WiMAX/WiFi Link 5350 and Intel® WiMAX/WiFi Link 5150

WiFi / WiMAX
Form Factor | PCI Express* Mini Card or Half-Mini Card
SKUs | Intel® WiMAX/WiFi Link 5350 - 3x3 MC Intel® WiMAX/WiFi Link 5150 - 1x2 MC/HMC
Dimensions | Mini Card: Width 2.0 in x Length 1.18 in x Height 0.18 in (50.80 mm x 30 mm x 4.5 mm) Half-Mini Card: Width 1.049 in x Length 1.18 in x Height 0.18 in (26.64 mm x 30 mm x 4.5 mm)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
Connector Interface | 53-pin Mini Card edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 90% non-condensing (at temperatures of 25 ºC to 35 ºC)
WiFi
Frequency Modulation | 5 GHz (802.11a/n) | 2.4 GHz (802.11b/g/n)
Frequency band | 5.15 GHz - 5.85 GHz (dependent on country) | 2.41-2.474 GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5 GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | 4 to 12 (dependent on country) | Channel 1-11 (US only) Channel 1-13 (Japan, Europe)
IEEE 802.11n Data Rates | Intel® WiFi Link 5350 450, 405, 360, 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2 Mbps
Intel® WiFi Link 5150 300, 270, 243, 240, 180, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2 Mbps
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
WiFi General
Operating Systems | Microsoft Windows* XP (32-bit and 64-bit) Windows Vista* (32-bit and 64-bit) Windows* 7 (32-bit and 64-bit)
Wi-Fi Alliance* certification | Wi-Fi* certification for 802.11b, 802.11g, 802.11a, 802.11h, 802.11d, WPA-Personal, WPA-Enterprise, WPA2-Personal, WPA2-Enterprise, WMM, WMM Power Save, EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
WLAN Standard | IEEE 802.11g, 802.11b, 802.11a, 802.11n
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, 802.1X: EAP-SIM, LEAP, PEAP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Encryption | AES-CCMP 128-bit, WEP 128-bit and 64-bit, CKIP, TKIP
Product Safety | UL, C-UL, CB (IEC 60590)
WiMAX
Frequency band | 2.5-2.7 GHz (3A Profile)
Modulation | UL - QPSK, 16 QAM DL - QPSK, 16 QAM, 64 QAM
Wireless Medium | Duplex mode: TDD operations | Scalable OFDMA (SOFDMA): 512 and 1024 FFT
sub-carrier permutation: PUSC | Channel bandwidths: 5 MHz and 10 MHz
WiMAX Network Release Feature set | SPWG/NWG Release 1.0 SPWG/NWG Release 1.5
Rate Performance | 10 Mbps DL and 4 Mbps UL @ peak rate (OTA performance, 10MHz channel)
RF Transmitter Output Power | Compliance with Power class 2
WiMAX General
Operating Systems | Microsoft Windows* XP (32-bit and 64-bit) Windows Vista* (32-bit and 64-bit) Windows* 7 (32-bit and 64-bit)
Standard Compliance | 802.16e-2005 Corrigenda 2 (D4)
WiMAX System Profile Feature set | Mobile WiMAX release 1, Wave II Profile 3A
Security | Key Management Protocol (PKMv2)
Encryption | 128-bit CCMP (Counter-Mode/CBC-MAC) based on AES encryption

Back to Top

Back to Contents

Trademarks and Disclaimers