**
**
**  VIA PCI Card Reader Host Controller
**
**  WDM Driver for Windows XP/Svr2003/Vista x64 edition
**
**  v1.45   Dec, 2009
**
**

Introduction:
=============

  This document shows you how to setup the driver in Windows operating system.

Contents of the Subdirectory:
=============================

    VIACR64.SYS          The WDM x64 driver for Windows XP/Svr2003/Vista.
    VIACR64.INF          The installation information file.
    VIACR64.CAT          The WDM x64 driver Windows logo signature file.
    CRICON.DLL           The customized memory card drive icons dll file.
    VIACR64.TXT          This file.

Installation:
=============

  Before starting with the installation process, make sure that the adapter
  is properly installed and configured.

    1. Turn on the power of your PC to boot into Windows operating system.
       Windows will auto-detect your new hardware, and the "New Hardware Found"
       dialogue box will appear. Select "Driver from disk provided by hardware
       manufacturer" to install driver from the driver diskette or other location.

    2. When the driver installation is completed, restart Windows if needed.

