Follow these steps to upgrade BIOS:
1.	Open the chassis;
2.	Short Jumper JP7 on the board (position betweeen PCI2 and USB2 );
3.	Power on and boot DOS;
4.	Run Flash.BAT;
5.	Wait for BIOS upgrading process complete and power off;
6.	Keep JP7 Open then close chassis
The new BIOS was modified for the following reason:
    1.Support for Intel's next generation 22nm processors.


升級BIOS步驟:
    1.打開主機殼.
    2.短接主板上的JP7(在PCI2和USB2之間).
    3.開機並啟動到DOS.
    4.執行Flash.BAT.
    5.等待更新BIOS完畢後關機.
    6.斷開JP7.併合上主機殼.
新BIOS修改原因如下:
    1.支援英特爾下一代22納米處理器.

