;/*++
;
;Copyright (c) 2001-2006 Atheros Communications, Incorporated All Rights Reserved
;
;Module Name:
;
;    netathw.inf
;
;Abstract:
;    INF file for installing Atheros AR5008 Wireless Network Adapter
;
;    Installs athw.sys (NDIS 5/5.1 driver) on NT platforms (2000, XP and greater)
;    Installs athwx.sys (NDIS 5 driver) on 9x platforms
;
;--*/

[Version]
Signature   = "$CHICAGO$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %ATHEROS%
Compatible  = 1
DriverVer   = 04/01/2008,7.4.2.105
Catalogfile.nt = netathw.cat
;Catalogfile = netathw.cat

[Manufacturer]
%ATHEROS%     = Atheros
%Gigabyte%    = Gigabyte

[ControlFlags]
ExcludeFromSelect = \  ;for win95 and legacy support
  PCI\VEN_168C&DEV_0013

[Atheros]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
; Generic
%ATHER.DeviceDesc.0013%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013
%ATHER.DeviceDesc.0013%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_0014
%ATHER.DeviceDesc.0013%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_0015
%ATHER.DeviceDesc.0013%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_0016
%ATHER.DeviceDesc.0013%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_0017
%ATHER.DeviceDesc.0013%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_0018
%ATHER.DeviceDesc.0013%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_0019
%ATHER.DeviceDesc.001A%  = ATHER_DEV_001A.ndi,    PCI\VEN_168C&DEV_001A
%ATHER.DeviceDesc.001B%  = ATHER_DEV_001B.ndi,    PCI\VEN_168C&DEV_001B
%ATHER.DeviceDesc.001B%  = ATHER_DEV_001B.ndi,    PCI\VEN_168C&DEV_001C
%ATHER.DeviceDesc.001B%  = ATHER_DEV_001B.ndi,    PCI\VEN_168C&DEV_FF19
%ATHER.DeviceDesc.001D%  = ATHER_DEV_001D.ndi,    PCI\VEN_168C&DEV_001D
%ATHER.DeviceDesc.0023%  = ATHER_DEV_0023.ndi,    PCI\VEN_168C&DEV_0023
%ATHER.DeviceDesc.0023%  = ATHER_DEV_0023.ndi,    PCI\VEN_168C&DEV_0024
%ATHER.DeviceDesc.0023%  = ATHER_DEV_0023.ndi,    PCI\VEN_168C&DEV_FF1C
%ATHER.DeviceDesc.0023%  = ATHER_DEV_0023.ndi,    PCI\VEN_168C&DEV_FF1D

; Atheros
%ATHER.DeviceDesc.1025%  = ATHER_DEV_1025.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1025168C
%ATHER.DeviceDesc.2025%  = ATHER_DEV_2025.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2025168C
%ATHER.DeviceDesc.1026%  = ATHER_DEV_1026.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1026168C
%ATHER.DeviceDesc.2026%  = ATHER_DEV_2026.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2026168C
%ATHER.DeviceDesc.1027%  = ATHER_DEV_1027.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1027168C
%ATHER.DeviceDesc.2027%  = ATHER_DEV_2027.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2027168C
%ATHER.DeviceDesc.1030%  = ATHER_DEV_1030.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1030168C
%ATHER.DeviceDesc.2030%  = ATHER_DEV_2030.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2030168C
%ATHER.DeviceDesc.1031%  = ATHER_DEV_1031.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1031168C
%ATHER.DeviceDesc.2031%  = ATHER_DEV_2031.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2031168C
%ATHER.DeviceDesc.1041%  = ATHER_DEV_1041.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1041168C
%ATHER.DeviceDesc.2041%  = ATHER_DEV_2041.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2041168C
%ATHER.DeviceDesc.1042%  = ATHER_DEV_1042.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1042168C
%ATHER.DeviceDesc.2042%  = ATHER_DEV_2042.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2042168C
%ATHER.DeviceDesc.1051%  = ATHER_DEV_1051.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1051168C
%ATHER.DeviceDesc.2051%  = ATHER_DEV_2051.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2051168C
%ATHER.DeviceDesc.001A%  = ATHER_DEV_1052.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_1052168C
%ATHER.DeviceDesc.001A%  = ATHER_DEV_2052.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_2052168C
%ATHER.DeviceDesc.1053%  = ATHER_DEV_1053.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1053168C
%ATHER.DeviceDesc.2053%  = ATHER_DEV_2053.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2053168C
%ATHER.DeviceDesc.001A%  = ATHER_DEV_1054.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_1054168C
%ATHER.DeviceDesc.001A%  = ATHER_DEV_2054.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_2054168C
%ATHER.DeviceDesc.1062%  = ATHER_DEV_1062.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_1062168C
%ATHER.DeviceDesc.2062%  = ATHER_DEV_2062.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_2062168C
%ATHER.DeviceDesc.001B%  = ATHER_DEV_1063.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_1063168C
%ATHER.DeviceDesc.001B%  = ATHER_DEV_2063.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_2063168C
%ATHER.DeviceDesc.3062%  = ATHER_DEV_2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_3062168c
%ATHER.DeviceDesc.3063%  = ATHER_DEV_2063.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_3063168c
%ATHER.DeviceDesc.3061%  = ATHER_DEV_2051.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_3061168c
%ATHER.DeviceDesc.3065%  = ATHER_DEV_2052.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_3065168c
%ATHER.DeviceDesc.2061%  = ATHER_DEV_2051.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_2061168c
%ATHER.DeviceDesc.1061%  = ATHER_DEV_1051.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_1061168c
%ATHER.DeviceDesc.2065%  = ATHER_DEV_2052.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_2065168c
%ATHER.DeviceDesc.1065%  = ATHER_DEV_1052.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_1065168c
%ATHER.DeviceDesc.3067%  = ATHER_DEV_001C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_3067168C
%ATHER.DeviceDesc.3067%  = ATHER_DEV_001C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_3064168C
%ATHER.DeviceDesc.2055%  = ATHER_DEV_2055.ndi,    PCI\VEN_168C&DEV_001D&SUBSYS_2055168c
%ATHER.DeviceDesc.1055%  = ATHER_DEV_1055.ndi,    PCI\VEN_168C&DEV_001D&SUBSYS_1055168c

; Others
%ATHER.DeviceDesc.2026%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_7005144F
%ATHER.DeviceDesc.2026%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_7057144F
%ATHER.DeviceDesc.2026%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_7058144F
%ATHER.DeviceDesc.2041%  = ATHER_DEV_2041.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_7064144F
%ATHER.DeviceDesc.2042%  = ATHER_DEV_2042.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_7065144F
%ATHER.DeviceDesc.2051%  = ATHER_DEV_2051.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_7084144F
%ATHER.DeviceDesc.2051%  = ATHER_DEV_2051.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_7088144F
%ATHER.DeviceDesc.2062%  = ATHER_DEV_2062.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_7092144F
%ATHER.DeviceDesc.001A%  = ATHER_DEV_2054.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7094144F
%ATHER.DeviceDesc.2042%  = ATHER_DEV_2042.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_7005168C
%ATHER.DeviceDesc.3063%  = ATHER_DEV_2063.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7096144F
%ATHER.DeviceDesc.3065%  = ATHER_DEV_2052.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7106144F
%ATHER.DeviceDesc.3067%  = ATHER_DEV_001C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7128144f
%ATHER.DeviceDesc.0013%  = ATHER_DEV_F013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_123410CF
%ATHER.DeviceDesc.0013%  = ATHER_DEV_F013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_123510CF
%ATHER.DeviceDesc.10CF%  = ATHER_DEV_F013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_123610CF
%ATHER.DeviceDesc.001B%  = ATHER_DEV_F013.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_132910CF
%ATHER.DeviceDesc.10CF%  = ATHER_DEV_F013.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_134F10CF
%ATHER.DeviceDesc.3062%  = ATHER_DEV_F013.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_139C10CF
%ATHER.DeviceDesc.3067%  = ATHER_DEV_001C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_142E10CF
%ATHER.DeviceDesc.3062%  = ATHER_DEV_04221468.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_04221468
%ATHER.DeviceDesc.001A%  = ATHER_DEV_04171468.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_04171468
%ATHER.DeviceDesc.001A%  = ATHER_DEV_04171468.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_04181468
%ATHER.DeviceDesc.001A%  = ATHER_DEV_04171468.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_04201468
%ATHER.DeviceDesc.3067%  = ATHER_DEV_042A1468.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_042A1468
%ATHER.DeviceDesc.E000%  = ATHER_DEV_E000105B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_E000105B
%ATHER.DeviceDesc.E000%  = ATHER_DEV_E002105B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_E002105B
%ATHER.DeviceDesc.0406%  = ATHER_DEV_04061468.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_04061468
%ATHER.DeviceDesc.0407%  = ATHER_DEV_04071468.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_04071468
%ATHER.DeviceDesc.E000%  = ATHER_DEV_04231468.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_04231468
%ATHER.DeviceDesc.E000%  = ATHER_DEV_04231468.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_0423168C
%ATHER.DeviceDesc.3063%  = ATHER_DEV_2063.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_04271468
%ATHER.DeviceDesc.3065%  = ATHER_DEV_2052.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_04251468
%ATHER.DeviceDesc.001A%  = ATHER_DEV_2052.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_04261468
%ATHER.DeviceDesc.3067%  = ATHER_DEV_001C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_042A1468
%ATHER.DeviceDesc.0055%  = ATHER_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_123610CF
%ATHER.DeviceDesc.0055%  = ATHER_DEV_001B.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_134f10CF
%ATHER.DeviceDesc.3072%  = ATHER_DEV_13C010CF.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_13C010CF
%ATHER.DeviceDesc.3072%  = ATHER_DEV_7125144F.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_7125144F
%ATHER.DeviceDesc.3072%  = ATHER_DEV_7125144F.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_04291468
%ATHER.DeviceDesc.3072%  = ATHER_DEV_0023.ndi,        PCI\VEN_168C&DEV_0024&SUBSYS_04301468
%ATHER.DeviceDesc.3072%  = ATHER_DEV_05021A32.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_05021A32
%ATHER.DeviceDesc.3065%  = ATHER_DEV_01001A32.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_01001A32
%ATHER.DeviceDesc.3063%  = ATHER_DEV_02001A32.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_02001A32
%ATHER.DeviceDesc.3067%  = ATHER_DEV_01051A32.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_01051A32
%ATHER.DeviceDesc.3062%  = ATHR_DEV_N2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_102010E9
%ATHER.DeviceDesc.3062%  = ATHR_DEV_N2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_102510E9
%ATHER.DeviceDesc.3072%  = ATHR_DEV_N3072.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_102210E9
%ATHER.DeviceDesc.3072%  = ATHR_DEV_N3073.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_102610E9
; Acer
%ATHER.DeviceDesc.3067%  = ATHER_DEV_04281468.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_04281468
%ATHER.DeviceDesc.3067%  = ATHER_DEV_04281468.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_E008105B
; Lenovo Japan
%ATHER.DeviceDesc.5013%  = ATHER_DEV_5013.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_0034168c
%ATHER.DeviceDesc.6013%  = ATHER_DEV_6013.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_0035168c
%ATHER.DeviceDesc.3013%  = ATHER_DEV_3013.ndi,    PCI\VEN_168C&DEV_1014&SUBSYS_05891014
%ATHER.DeviceDesc.4013%  = ATHER_DEV_4013.ndi,    PCI\VEN_168C&DEV_1014&SUBSYS_058A1014
%ATHER.DeviceDesc.2013%  = ATHER_DEV_2013.ndi,    PCI\VEN_168C&DEV_1014&SUBSYS_057E1014
%ATHER.DeviceDesc.1013%  = ATHER_DEV_1013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_04081468
%ATHER.DeviceDesc.0032168c% = ATHER_DEV_0032168c.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_0032168c
%ATHER.DeviceDesc.0033168c% = ATHER_DEV_0033168c.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_0033168c
%ATHER.DeviceDesc.0033168c% = ATHER_DEV_7125144F.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_03841014
; Samsung
%ATHER.DeviceDesc.001A%  = ATHER_DEV_S001A.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_7101144F
%ATHER.DeviceDesc.001A%  = ATHER_DEV_S001A.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_7114144F
%ATHER.DeviceDesc.001A%  = ATHER_DEV_S001A.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_7115144F
%ATHER.DeviceDesc.3067%  = ATHER_DEV_S3067a.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7131144F
%ATHER.DeviceDesc.3067%  = ATHER_DEV_S3067a.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7130144F
%ATHER.DeviceDesc.001B%  = ATHER_DEV_S001B.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7108144F
%ATHER.DeviceDesc.001B%  = ATHER_DEV_S001B.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7116144F
; D-Link
%ATHER.DeviceDesc.DWA642%   = ATHER_DEV_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A6A1186
%ATHER.DeviceDesc.DWA645%   = ATHER_DEV_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A0907D1
%ATHER.DeviceDesc.DWA645%   = ATHER_DEV_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A761186
%ATHER.DeviceDesc.DWA542%   = ATHER_DEV_3A691186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A691186
%ATHER.DeviceDesc.DWA547%   = ATHER_DEV_3A6D1186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A6B1186
%ATHER.DeviceDesc.DWA652%   = ATHER_DEV_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A6E1186
%ATHER.DeviceDesc.DWA552%   = ATHER_DEV_3A6D1186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A6D1186
%ATHER.DeviceDesc.DWA643%   = ATHER_DEV_3A6F1186.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_3A6F1186
%ATHER.DeviceDesc.DWA556%   = ATHER_DEV_3A701186.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_3A701186
%ATHER.DeviceDesc.DWA520%   = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A731186
%ATHER.DeviceDesc.DWA620%   = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A741186
%ATHER.DeviceDesc.WDA1320%  = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A1D1186
%ATHER.DeviceDesc.WDA2320%  = ATHER_DEV_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A1B1186
%ATHER.DeviceDesc.WNA2330%  = ATHER_DEV_WNA2330.ndi,  PCI\VEN_168C&DEV_0013&SUBSYS_3A1A1186
%ATHER.DeviceDesc.WNA1330%  = ATHER_DEV_WNA1330.ndi,  PCI\VEN_168C&DEV_001A&SUBSYS_3A1C1186
; Toshiba
%ATHER.DeviceDesc.3067%     = ATHER_DEV_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_41051A32
; Alpha/ATKK
%ATIWC.DeviceDesc.ATICB%  = ATHER_DEV_0013.ndi,	PCI\VEN_168C&DEV_0013&SUBSYS_12041259
%ATIWC.DeviceDesc.ATIPC%  = ATHER_DEV_0013.ndi,	PCI\VEN_168C&DEV_0013&SUBSYS_12031259
; Motion Computing
%ATHER.DeviceDesc.3062%  = ATHER_DEV_7111144F.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7111144F
; Azurewave
%ATHER.DeviceDesc.3067%  = ATHER_DEV_10261A3B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_10261A3B
%ATHER.DeviceDesc.3067%  = ATHER_DEV_10261A3B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_10601A3B
%ATHER.DeviceDesc.0024%     = ATHER_DEV_10241A3B.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_10241A3B
;LiteOn
%ATHER.DeviceDesc.3067%     = ATHER_DEV_6313.ndi,        PCI\VEN_168C&DEV_001C&SUBSYS_630311AD
%ATHER.DeviceDesc.3067%     = ATHER_DEV_6313.ndi,        PCI\VEN_168C&DEV_001C&SUBSYS_631311AD
[Gigabyte]
%GIGA.DeviceDesc.E801%  = GIGA_DEV_E801.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_E8011458
%GIGA.DeviceDesc.E811%  = GIGA_DEV_E811.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_E8111458
%GIGA.DeviceDesc.E814%  = GIGA_DEV_E814.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_E8141458
%GIGA.DeviceDesc.0013%  = GIGA_DEV_0013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_E9011458
%GIGA.DeviceDesc.E901%  = GIGA_DEV_E901.ndi,    PCI\VEN_168C&DEV_001B&SUBSYS_E9011458
%GIGA.DeviceDesc.E911%  = GIGA_DEV_E911.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_E9111458
%GIGA.DeviceDesc.E912%  = GIGA_DEV_E912.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_E9121458
%GIGA.DeviceDesc.E913%  = GIGA_DEV_E913.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_E9131458
%GIGA.DeviceDesc.E917%  = GIGA_DEV_E917.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_E9171458
%GIGA.DeviceDesc.E815%  = GIGA_DEV_E914.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_E8151458
%GIGA.DeviceDesc.E914%  = GIGA_DEV_E914.ndi,    PCI\VEN_168C&DEV_0023&SUBSYS_E9141458
%GIGA.DeviceDesc.E915%  = GIGA_DEV_E914.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_E9151458
%GIGA.DeviceDesc.E916%  = GIGA_DEV_E916.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_E9161458
%GIGA.DeviceDesc.E918%  = GIGA_DEV_E918.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_E9181458

; Remark whole Win9x Section since Win98/Win98se/WinMe is no longer supported
; This section to be deleted
; Windows 9X specific entries

;[ATHER_DEV_0013.ndi]
;AddReg          = ATHER_DEV_0013.id.reg, 5211.reg, ATHER.win.reg, 5212.abgcb.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_001A.ndi]
;AddReg          = ATHER_DEV_001A.id.reg, 5211.reg, ATHER.win.reg, 5212.bgcb.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_001B.ndi]
;AddReg          = ATHER_DEV_001B.id.reg, 5211.reg, ATHER.win.reg, 5212.abgcb.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_1025.ndi]
;AddReg          = ATHER_DEV_1025.id.reg, 5211.reg, ATHER.win.reg, 5212.bgcb.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_2025.ndi]
;AddReg          = ATHER_DEV_2025.id.reg, 5211.reg, ATHER.win.reg, 5212.bgmp.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_1026.ndi]
;AddReg          = ATHER_DEV_1026.id.reg, 5211.reg, ATHER.win.reg, 5212.abgcb.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_2026.ndi]
;AddReg          = ATHER_DEV_2026.id.reg, 5211.reg, ATHER.win.reg, 5212.abgmp.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_1027.ndi]
;AddReg          = ATHER_DEV_1027.id.reg, 5211.reg, ATHER.win.reg, 5212.bgcb.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_2027.ndi]
;AddReg          = ATHER_DEV_2027.id.reg, 5211.reg, ATHER.win.reg, 5212.bgmp.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_1030.ndi]
;AddReg          = ATHER_DEV_1030.id.reg, 5211.reg, ATHER.win.reg, 5212.bgcb.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_2030.ndi]
;AddReg          = ATHER_DEV_2030.id.reg, 5211.reg, ATHER.win.reg, 5212.bgmp.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_1031.ndi]
;AddReg          = ATHER_DEV_1031.id.reg, 5211.reg, ATHER.win.reg, 5212.abgcb.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_2031.ndi]
;AddReg          = ATHER_DEV_2031.id.reg, 5211.reg, ATHER.win.reg, 5212.abgmp.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_1041.ndi]
;AddReg          = ATHER_DEV_1041.id.reg, 5211.reg, ATHER.win.reg, 5212.bgcb.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_2041.ndi]
;AddReg          = ATHER_DEV_2041.id.reg, 5211.reg, ATHER.win.reg, 5212.bgmp.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_1042.ndi]
;AddReg          = ATHER_DEV_1042.id.reg, 5211.reg, ATHER.win.reg, 5212.abgcb.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_2042.ndi]
;AddReg          = ATHER_DEV_2042.id.reg, 5211.reg, ATHER.win.reg, 5212.abgmp.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_1051.ndi]
;AddReg          = ATHER_DEV_1051.id.reg, 5211.reg, ATHER.win.reg, 5212.bgcb.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_1052.ndi]
;AddReg          = ATHER_DEV_1052.id.reg, 5211.reg, ATHER.win.reg, 5212.bgcb.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_1053.ndi]
;AddReg          = ATHER_DEV_1053.id.reg, 5211.reg, ATHER.win.reg, 5212.bgcb.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_1054.ndi]
;AddReg          = ATHER_DEV_1054.id.reg, 5211.reg, ATHER.win.reg, 5212.bgcb.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_2051.ndi]
;AddReg          = ATHER_DEV_2051.id.reg, 5211.reg, ATHER.win.reg, 5212.bgmp.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_2052.ndi]
;AddReg          = ATHER_DEV_2052.id.reg, 5211.reg, ATHER.win.reg, 5212.bgmp.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_001C.ndi]
;AddReg          = ATHER_DEV_001C.id.reg, 5211.reg, ATHER.win.reg, 5212.bgmp.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_2053.ndi]
;AddReg          = ATHER_DEV_2053.id.reg, 5211.reg, ATHER.win.reg, 5212.bgmp.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_2054.ndi]
;AddReg          = ATHER_DEV_2054.id.reg, 5211.reg, ATHER.win.reg, 5212.bgmp.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_1062.ndi]
;AddReg          = ATHER_DEV_1062.id.reg, 5211.reg, ATHER.win.reg, 5212.abgcb.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_1063.ndi]
;AddReg          = ATHER_DEV_1063.id.reg, 5211.reg, ATHER.win.reg, 5212.abgcb.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_2062.ndi]
;AddReg          = ATHER_DEV_2062.id.reg, 5211.reg, ATHER.win.reg, 5212.abgmp.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_04221468.ndi]
;AddReg          = ATHER_DEV_04221468.id.reg, 5211.reg, ATHER.win.reg, 5212.abgmp.reg, customer3.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_04171468.ndi]
;AddReg          = ATHER_DEV_04171468.id.reg, 5211.reg, ATHER.win.reg, 5212.bgmp.reg, customer3.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_2063.ndi]
;AddReg          = ATHER_DEV_2063.id.reg, 5211.reg, ATHER.win.reg, 5212.abgmp.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_F013.ndi]
;AddReg          = ATHER_DEV_0013.id.reg, 5211.reg, ATHER.win.reg, 5212.abgcb.reg, customer1ani.reg, bandselect.reg 
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_001D.ndi]
;AddReg          = ATHER_DEV_001D.id.reg, 5211.reg, ATHER.win.reg, 5212.bgcb.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_1055.ndi]
;AddReg          = ATHER_DEV_1055.id.reg, 5211.reg, ATHER.win.reg, 5212.bgcb.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_2055.ndi]
;AddReg          = ATHER_DEV_2055.id.reg, 5211.reg, ATHER.win.reg, 5212.bgmp.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

;[ATHER_DEV_0023.ndi]
;AddReg          = ATHER_DEV_0023.id.reg, 5416.reg, ATHER.win.reg, 5416.abgncb.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5416.DelReg

;[ATHER_DEV_0033168c.ndi]
;AddReg          = ATHER_DEV_0023.id.reg, 5416.reg, ATHER.win.reg, 5416.abgnxb.reg, customer0.reg, 5416.antennacontrols.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5416.DelReg

;[ATHER_DEV_0032168c.ndi]
;AddReg          = ATHER_DEV_0023.id.reg, 5416.reg, ATHER.win.reg, 5416.bgnxb.reg, customer0.reg, 5416.antennacontrols.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5416.DelReg

;[ATHER_DEV_13C010CF.ndi]
;AddReg          = ATHER_DEV_0023.id.reg, 5416.reg, ATHER.win.reg, 5416.abgnxb.reg, 5416.antennacontrols.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5416.DelReg

;[ATHER_DEV_7125144F.ndi]
;AddReg          = ATHER_DEV_0023.id.reg, 5416.reg, ATHER.win.reg, 5416.abgncb.reg, 5416.antennacontrols.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5416.DelReg

;[ATHR_DEV_N2062.ndi]
;Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
;BusType         = 5
;DelReg          = 5211.DelReg
;AddReg          = customer11.reg, customer11_legacywmode.reg, customer11Led.reg, customer11Ant.reg, ATHER.reg, customer11ACStatus.reg
;CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles

;[ATHR_DEV_N3072.ndi]
;Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
;BusType         = 5
;DelReg          = 5416.DelReg
;AddReg          = customer11.reg, customer11_11nwmode.reg, customer11Led.reg, ATHER.reg, sys.TcpParams.reg, customer11ACStatus.reg
;CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles

;[ATHR_DEV_N3073.ndi]
;Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
;BusType         = 5
;DelReg          = 5416.DelReg
;AddReg          = customer11.reg, customer11_11n40wmode.reg, customer11Led.reg, ATHER.reg, sys.TcpParams.reg, customer11ACStatus.reg
;CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles

;[GIGA_DEV_E914.ndi]
;AddReg          = GIGA_DEV_E914.id.reg, customer12Led0.reg, 5416.reg, ATHER.win.reg, 5416.abgncb.reg, customer12.reg, 5416.antennacontrols.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5416.DelReg

;[GIGA_DEV_E916.ndi]
;AddReg          = GIGA_DEV_E914.id.reg, customer12Led1.reg, 5416.reg, ATHER.win.reg, 5416.abgncb.reg, customer12.reg, 5416.antennacontrols.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5416.DelReg

;[GIGA_DEV_E918.ndi]
;AddReg          = GIGA_DEV_E918.id.reg, customer12led2.reg, 5211.reg, ATHER.win.reg, 5212.bgmp.reg
;CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DelFiles        = ATHER.DelIniFiles
;DelReg          = 5211.DelReg

; Remark whole Win9x Section since Win98/Win98se/WinMe is no longer supported


; Windows NT specific entries

[ATHER_DEV_0013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_001A.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_001B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1025.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2025.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1026.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2026.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1027.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2027.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1030.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2030.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1031.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2031.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1041.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2041.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1051.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2051.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1042.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2042.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1052.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2052.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_001C.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_6313.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, uapsd.reg, customer6Led.reg, d3hot.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1053.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2053.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1054.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2054.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1062.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2062.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_7111144F.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, Customer14.led.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_04221468.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.abgmp.reg, customer3.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_04171468.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, customer3.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_04281468.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.abgmp.reg, customer3a.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_01001A32.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, customer10.LED3.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_02001A32.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.abgmp.reg, customer10.LED3.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_01051A32.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.abgmp.reg, customer3a.reg, uapsd.reg, d3hot.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_042A1468.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, customer9.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E000105B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, customer4b.reg, customer4_basic.reg, customer4a_ASPM.reg, uapsd.reg, d3hot.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_E002105B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, customer4b.reg, customer4_basic.reg, customer4a_ASPM.reg, uapsd.reg, d3hot.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_04061468.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, customer4a.reg,customer4_basic.reg, customer4a_ASPM.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_04071468.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, COMMON_AG.reg, customer4a.reg,customer4_basic.reg, customer4a_ASPM.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_04231468.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, customer4a.reg,customer4_basic.reg, customer4a_ASPM.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_10261A3B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, 10261a3b.reg, uapsd.reg, d3hot.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1063.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2063.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_F013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.abgcb.reg, customer1ani.reg, bandselect.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_001D.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1055.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2055.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, customer0.PS1.reg, customer0.LED.reg, customer0.5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, customer0.PS1.reg, customer0.LED1.reg, customer0.5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, customer0.PS1.reg, customer0.LED.reg, customer0.5213.abg.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_4013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, customer0.PS1.reg, customer0.LED1.reg, customer0.5213.abg.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_5013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, customer0.PS1.reg, customer0.LED2.reg, customer0.5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_6013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer0.5211.reg, ATHER.reg, customer0.PS1.reg, customer0.LED2.reg, customer0.5212.bgmp.reg, uapsd.reg, d3hot.reg
CopyFiles       = ATHER.CopyFiles.nt
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_0023.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.abgncb.reg, sys.TcpParams.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_05021A32.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.abgncb.reg, sys.TcpParams.reg, customer10.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_0033168c.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.abgnxb.reg, sys.TcpParams.reg, customer0.reg, 5416.antennacontrols.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_0032168c.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.bgnxb.reg, sys.TcpParams.reg, customer0.reg, 5416.antennacontrols.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_13C010CF.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.abgnxb.reg, sys.TcpParams.reg, 5416.antennacontrols.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_7125144F.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, 5416.abgncb.reg, sys.TcpParams.reg, 5416.antennacontrols.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E801.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5211.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E811.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5211.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E814.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5211.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_0013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5211.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E901.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5211.reg, 5212.abgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E911.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5211.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E912.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led0.reg, 5211.reg, ATHER.reg, 5211.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E913.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led1.reg, 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E917.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led1.reg, 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E918.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer12led2.reg, 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E914.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, customer12Led0.reg, 5416.reg, 5416.abgncb.reg, sys.TcpParams.reg, 5416.antennacontrols.reg, customer12.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[GIGA_DEV_E916.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, customer12Led1.reg, 5416.reg, 5416.abgncb.reg, sys.TcpParams.reg, 5416.antennacontrols.reg, customer12.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHR_DEV_N2062.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = customer11.reg, customer11_legacywmode.reg, customer11Led.reg, customer11Ant.reg, ATHER.reg, customer11ACStatus.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHR_DEV_N3072.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = customer11.reg, customer11_11nwmode.reg, customer11Led.reg, ATHER.reg, sys.TcpParams.reg, customer11ACStatus.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHR_DEV_N3073.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = customer11.reg, customer11_11n40wmode.reg, customer11Led.reg, ATHER.reg, sys.TcpParams.reg, customer11ACStatus.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1186.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, sys.TcpParams.reg, customer5.11nLED.reg, customer5.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3A691186.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, sys.TcpParams.reg, customer5.11nLED.reg, pcibusconfig.reg, customer5.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3A6D1186.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, sys.TcpParams.reg, customer5.11nLED.reg, pcibusconfig.reg, customer5.3x3.reg, customer5.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3A6F1186.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, sys.TcpParams.reg, customer5.PCIe11nLed.reg, customer5.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_3A701186.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, sys.TcpParams.reg, customer5.PCIe11nLed.reg, customer5.3x3.reg, customer5.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_WNA2330.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgcb.reg, wnaled.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_WNA1330.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgcb.reg, wnaled.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_S001A.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_S001B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.abgcb.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_S3067a.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5211.DelReg
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.bgmp.reg, customer_Samsung.reg, rssiAdjust.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_10241A3B.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = 5416.DelReg
AddReg          = 5416.reg, ATHER.reg, 5416.reg, sys.TcpParams.reg, customer1a3b.reg, uapsd.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_05021A32.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_0013.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_001A.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_001B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1025.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2025.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1026.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2026.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1027.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2027.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1030.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2030.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1031.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2031.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1041.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2041.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1042.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2042.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1051.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2051.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1052.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2052.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_001C.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_6313.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1053.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2053.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1054.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2054.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1062.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2062.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_7111144F.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_04221468.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_04171468.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1063.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_F013.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_001D.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1055.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2055.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1013.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3013.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2013.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_4013.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_5013.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_6013.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_0023.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_0033168c.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_0032168c.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_13C010CF.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_7125144F.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_04281468.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_01051A32.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_042A1468.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E000105B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_E002105B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_04061468.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_04071468.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_04231468.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2063.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_10261A3B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_01001A32.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_02001A32.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHR_DEV_N2062.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHR_DEV_N3072.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHR_DEV_N3073.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E801.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E811.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E814.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_0013.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E901.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E911.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E912.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E913.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E917.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E918.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E914.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[GIGA_DEV_E916.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1186.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3A691186.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3A6D1186.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3A6F1186.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_3A701186.NDI.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_WNA2330.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_WNA1330.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_S001A.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_S001B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_S3067a.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

[ATHER_DEV_10241A3B.ndi.NT.Services]
AddService      = AR5416, 2, ATHER.Service, common.EventLog

;----------------------------------------------------------------------------
; Remark whole Win9x Section since Win98/Win98se/WinMe is no longer supported
; This section to be deleted
; Win9x id registry sections
; These are not needed by NT

;[ATHER_DEV_0013.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013"

;[ATHER_DEV_001A.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001A"

;[ATHER_DEV_001B.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001B"

;[ATHER_DEV_1025.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_1025168C"

;[ATHER_DEV_2025.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_2025168C"

;[ATHER_DEV_1026.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_1026168C"

;[ATHER_DEV_2026.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_2026168C"

;[ATHER_DEV_1027.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_1027168C"

;[ATHER_DEV_2027.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_2027168C"

;[ATHER_DEV_1030.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_1030168C"

;[ATHER_DEV_2030.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_2030168C"

;[ATHER_DEV_1031.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_1031168C"

;[ATHER_DEV_2031.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_2031168C"

;[ATHER_DEV_1041.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_1041168C"

;[ATHER_DEV_2041.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_2041168C"

;[ATHER_DEV_1042.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_1042168C"

;[ATHER_DEV_2042.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_2042168C"

;[ATHER_DEV_1051.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_1051168C"

;[ATHER_DEV_1052.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001A&SUBSYS_1052168C"

;[ATHER_DEV_1053.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_1053168C"

;[ATHER_DEV_1054.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001A&SUBSYS_1054168C"

;[ATHER_DEV_2051.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_2051168C"

;[ATHER_DEV_2052.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001A&SUBSYS_2052168C"

;[ATHER_DEV_001C.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001C&SUBSYS_3067168C"

;[ATHER_DEV_2053.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_2053168C"

;[ATHER_DEV_2054.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001A&SUBSYS_2054168C"

;[ATHER_DEV_1062.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001B&SUBSYS_1062168C"

;[ATHER_DEV_2062.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001B&SUBSYS_2062168C"

;[ATHER_DEV_04221468.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001C&SUBSYS_04221468"

;[ATHER_DEV_04171468.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001C&SUBSYS_04171468"

;[ATHER_DEV_1063.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001B&SUBSYS_1063168C"

;[ATHER_DEV_2063.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001B&SUBSYS_2063168C"

;[ATHER_DEV_F013.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013"

;[ATHER_DEV_001D.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001D"

;[ATHER_DEV_1055.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001D&SUBSYS_1055168C"

;[ATHER_DEV_2055.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001D&SUBSYS_2055168C"

;[ATHER_DEV_0023.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0023"

;[GIGA_DEV_E914.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0023&SUBSYS_E9141458"

;[GIGA_DEV_E918.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001C&SUBSYS_E9181458"

;[ATHER_DEV_WNA2330.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_3A1A1186"

;[ATHER_DEV_WNA1330.id.reg]
;HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001A&SUBSYS_3A1C1186"

;
; 5211 Enumerated Types
;

[5212.abgcb.reg]
HKR, ,                                  NetBand,                        0x00002,  "1823"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1

[5212.abgmp.reg]
HKR, ,                                  NetBand,                        0x00002,  "1823"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  2

[5212.bgcb.reg]
HKR, ,                                  NetBand,                        0x00002,  "28"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1

[5212.bgmp.reg]
HKR, ,                                  NetBand,                        0x00002,  "28"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  2

[5416.abgncb.reg]
HKR, ,                                  NetBand,                        0x00002,  "61455"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, ,                                  rmEnable,                       0x00002,  "1"
HKR, ,                                  abolt,                          0x00002,  "0"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[5416.bgnxb.reg]
HKR, ,                                  NetBand,                        0x00002,  "40972"
HKR, ,                                  wModeSelect,                    0x00002,  "40972"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, ,                                  abolt,                          0x00002,  "0"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                                  rmEnable,                       0x00002,  "1"

[5416.abgnxb.reg]
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, ,                                  abolt,                          0x00002,  "0"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                                  rmEnable,                       0x00002,  "1"
HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "61455"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "61455",                        0,  "Auto"
HKR, Ndi\params\NetBand\enum,           "20481",                        0,  "5Ghz Only"
HKR, Ndi\params\NetBand\enum,           "40972",                        0,  "2.4Ghz Only"

[5416.antennacontrols.reg] 
HKR, ,                                  rxChainSelect,                 	0x00002,  "7"
;HKR, ,                                  txChainSelectLegacy,            0x00002,  "5"
HKR, ,                                  rxChainSelectLegacy,           	0x00002,  "7"
HKR, ,                                  forceBias,           	        0x00002,  "2"
HKR, ,                                  rxChainDetect,                  0x00002,  "1"
HKR, ,                                  rxChainDetectRef,               0x00002,  "0"
HKR, ,                                  rxChainDetectThreshA,           0x00002,  "0"
HKR, ,                                  rxChainDetectThreshG,           0x00002,  "0"
HKR, ,                                  rxChainDetectDeltaA,            0x00002,  "20"
HKR, ,                                  rxChainDetectDeltaG,            0x00002,  "20"

[bandselect.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,        %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,        "10"
HKR, Ndi\params\NetBand,                default,                        0,        "1823"
HKR, Ndi\params\NetBand,                type,                           0,        "enum"
HKR, Ndi\params\NetBand\enum,           "1823",                         0,        "Auto"
HKR, Ndi\params\NetBand\enum,           "1795",                         0,        "5Ghz Only"
HKR, Ndi\params\NetBand\enum,           "28",                           0,        "2.4Ghz Only"

[pcibusconfig.reg]
HKR, ,                                  BusConfig,                 	0x00002,  "0"

[d3hot.reg]
HKR, ,                                  pciePowerReset,                 0x00002,  "0"
HKR, ,                                  pcieRestore,                 	0x00002,  "1"

; Allow non admin uses to switch profiles
;[5211.reg.security]
;"D:ARAI(A;;GA;;;BA)(A;;GA;;;SY)(A;CI;GA;;;IU)"

;-----------------------------------------------------------------------------
;
; 5211 common
;
[5211.DelReg]
HKR,,NetBand
HKR,,ssid
HKR,,ssid2
HKR,,ssid3
HKR,,prefBssid1
HKR,,prefBssid2
HKR,,prefBssid3
HKR,,prefBssid4
HKR,Ndi\Params\tpc
HKR,,tpc
HKR,Ndi\Params\authTypeUseOnly
HKR,,authTypeUseOnly
HKR,,AdHocBand
HKR,,AwakeTimePerf
HKR,,beaconInterval
HKR,,bkScanEnable
HKR,,bssType
HKR,,ccode
HKR,,clist
HKR,,defaultKey
HKR,,EncryptionAlg
HKR,,FragThreshold
HKR,,HwTxRetries
HKR,,privacyInvoked
HKR,,QoS
HKR,,rateCtrlEnable
HKR,,RTSThreshold
HKR,,scanType
HKR,,SwTxRetryScale
HKR,,SmeEnable
HKR,,aifs
HKR,,cwmin
HKR,,pcieClockReq
HKR,Ndi\params\sleepMode
HKR,Ndi\params\sleepMode\enum
HKR, Ndi\params\ExtendedChannel
HKR, NDI\params\Mode11dSwitch
HKR, Ndi\params\MapRegisters
HKR, CustomParams\Configurations\Cfg0

[5211.reg]
HKR, Ndi\params\MapRegisters,           ParamDesc,                      0,  %MapRegisters%
HKR, Ndi\params\MapRegisters,           default,                        0,  "256"
HKR, Ndi\params\MapRegisters,           min,                            0,  "32"
HKR, Ndi\params\MapRegisters,           max,                            0,  "512"
HKR, Ndi\params\MapRegisters,           step,                           0,  "8"
HKR, Ndi\params\MapRegisters,           base,                           0,  "10"
HKR, Ndi\params\MapRegisters,           type,                           0,  "int"

HKR, Ndi\params\NetworkAddress,         ParamDesc,                      0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,         default,                        0,  ""
HKR, Ndi\params\NetworkAddress,         LimitText,                      0,  "12"
HKR, Ndi\params\NetworkAddress,         UpperCase,                      0,  "1"
HKR, Ndi\params\NetworkAddress,         optional,                       0,  "1"
HKR, Ndi\params\NetworkAddress,         type,                           0,  "edit"

HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "2"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  "1"
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,  %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,  "10"
HKR, Ndi\params\radioEnable,            default,                        0,  "1"
HKR, Ndi\params\radioEnable,            type,                           0,  "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,  %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,  %radioEnableOff%

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"

HKR, Ndi\params\ccx5FeatureEnable,      ParamDesc,                      0,  %ccx5FeatureEnable%
HKR, Ndi\params\ccx5FeatureEnable,      Base,                           0,  "10"
HKR, Ndi\params\ccx5FeatureEnable,      default,                        0,  "0"
HKR, Ndi\params\ccx5FeatureEnable,      type,                           0,  "enum"
HKR, Ndi\params\ccx5FeatureEnable\enum, "1",                            0,  %ccx5FeatureEnableMfpEnable%
HKR, Ndi\params\ccx5FeatureEnable\enum, "0",                            0,  %ccx5FeatureEnableMfpDisable%

HKR, CustomParams\Configurations,       MajorVersion,                   0x10003,  2
HKR, CustomParams\Configurations,       MinorVersion,                   0x10003,  0

HKR, CustomParams\Configurations,       SelectedConfigurationIndex,     0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationName,      0x00002,  "Default"

[uapsd.reg]
HKR, Ndi\params\uapsdEnabledBE,            ParamDesc,                      0,  %uapsdEnabledBE%
HKR, Ndi\params\uapsdEnabledBE,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledBE,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledBE,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledBE\enum,       "1",                            0,  %uapsdEnabledBEOn%
HKR, Ndi\params\uapsdEnabledBE\enum,       "0",                            0,  %uapsdEnabledBEOff%

HKR, Ndi\params\uapsdEnabledBK,            ParamDesc,                      0,  %uapsdEnabledBK%
HKR, Ndi\params\uapsdEnabledBK,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledBK,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledBK,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledBK\enum,       "1",                            0,  %uapsdEnabledBKOn%
HKR, Ndi\params\uapsdEnabledBK\enum,       "0",                            0,  %uapsdEnabledBKOff%

HKR, Ndi\params\uapsdEnabledVI,            ParamDesc,                      0,  %uapsdEnabledVI%
HKR, Ndi\params\uapsdEnabledVI,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledVI,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledVI,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledVI\enum,       "1",                            0,  %uapsdEnabledVIOn%
HKR, Ndi\params\uapsdEnabledVI\enum,       "0",                            0,  %uapsdEnabledVIOff%

HKR, Ndi\params\uapsdEnabledVO,            ParamDesc,                      0,  %uapsdEnabledVO%
HKR, Ndi\params\uapsdEnabledVO,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledVO,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledVO,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledVO\enum,       "1",                            0,  %uapsdEnabledVOOn%
HKR, Ndi\params\uapsdEnabledVO\enum,       "0",                            0,  %uapsdEnabledVOOff%

;-----------------------------------------------------------------------------
;
; 5416 common
;
[5416.DelReg]
HKR,,NetBand
HKR,,ssid
HKR,,ssid2
HKR,,ssid3
HKR,,prefBssid1
HKR,,prefBssid2
HKR,,prefBssid3
HKR,,prefBssid4
HKR,Ndi\Params\tpc
HKR,,tpc
HKR,Ndi\Params\authTypeUseOnly
HKR,,authTypeUseOnly
HKR,,AdHocBand
HKR,,AwakeTimePerf
HKR,,beaconInterval
HKR,,bkScanEnable
HKR,,bssType
HKR,,ccode
HKR,,clist
HKR,,defaultKey
HKR,,EncryptionAlg
HKR,,FragThreshold
HKR,,HwTxRetries
HKR,,privacyInvoked
HKR,,QoS
HKR,,rateCtrlEnable
HKR,,RTSThreshold
HKR,,scanType
HKR,,SwTxRetryScale
HKR,,SmeEnable
HKR,,aifs
HKR,,cwmin
HKR,,pcieClockReq
HKR,,rmEnable

[5416.reg]
HKR, Ndi\params\MapRegisters,           ParamDesc,                      0,  %MapRegisters%
HKR, Ndi\params\MapRegisters,           default,                        0,  "256"
HKR, Ndi\params\MapRegisters,           min,                            0,  "32"
HKR, Ndi\params\MapRegisters,           max,                            0,  "512"
HKR, Ndi\params\MapRegisters,           step,                           0,  "8"
HKR, Ndi\params\MapRegisters,           base,                           0,  "10"
HKR, Ndi\params\MapRegisters,           type,                           0,  "int"

HKR, Ndi\params\NetworkAddress,         ParamDesc,                      0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,         default,                        0,  ""
HKR, Ndi\params\NetworkAddress,         LimitText,                      0,  "12"
HKR, Ndi\params\NetworkAddress,         UpperCase,                      0,  "1"
HKR, Ndi\params\NetworkAddress,         optional,                       0,  "1"
HKR, Ndi\params\NetworkAddress,         type,                           0,  "edit"

HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "2"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  "1"
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,  %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,  "10"
HKR, Ndi\params\radioEnable,            default,                        0,  "1"
HKR, Ndi\params\radioEnable,            type,                           0,  "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,  %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,  %radioEnableOff%

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"

HKR, Ndi\params\ccx5FeatureEnable,      ParamDesc,                      0,  %ccx5FeatureEnable%
HKR, Ndi\params\ccx5FeatureEnable,      Base,                           0,  "10"
HKR, Ndi\params\ccx5FeatureEnable,      default,                        0,  "0"
HKR, Ndi\params\ccx5FeatureEnable,      type,                           0,  "enum"
HKR, Ndi\params\ccx5FeatureEnable\enum, "1",                            0,  %ccx5FeatureEnableMfpEnable%
HKR, Ndi\params\ccx5FeatureEnable\enum, "0",                            0,  %ccx5FeatureEnableMfpDisable%

HKR, CustomParams\Configurations,       MajorVersion,                   0x10003,  2
HKR, CustomParams\Configurations,       MinorVersion,                   0x10003,  0

HKR, CustomParams\Configurations,       SelectedConfigurationIndex,     0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationName,      0x00002,  "Default"

;-----------------------------------------------------------------------------
;;Customized Section

[customer0.reg]
;PCIe Related
HKR, ,                                  pcieAspm,                 	0x00002,  "2"
HKR, ,                                  pciePowerSaveEnable,            0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  forceWake,                 	0x00002,  "0"
HKR, ,                                  antennaSwitchSwap,              0x00002,  "1"
;LED Related
HKR, ,                                  gpioPinFunc1,                  0x00002,  "1"
;General Customer0
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR,NDI\params\ignore11dBeacon,ParamDesc,,	"11d Mode Switch"
HKR,NDI\params\ignore11dBeacon,type,,		"enum"
HKR,NDI\params\ignore11dBeacon,Default,,	"1"
HKR,NDI\params\ignore11dBeacon\enum,0,,		"Enable"
HKR,NDI\params\ignore11dBeacon\enum,1,,		"Disable"

HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,  %roamRssiA%
HKR, Ndi\params\roamRssiA,              default,                        0,  "15"
HKR, Ndi\params\roamRssiA,              min,                            0,  "1"
HKR, Ndi\params\roamRssiA,              max,                            0,  "95"
HKR, Ndi\params\roamRssiA,           	step,                           0,  "1"
HKR, Ndi\params\roamRssiA,           	base,                           0,  "10"
HKR, Ndi\params\roamRssiA,           	type,                           0,  "int"

HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "1"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"

[customer0.5212.bgmp.reg]
HKR, ,                                  NetBand,                        0x00002,  "1823"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  2

HKR,NDI\params\TransmitRate11g,ParamDesc,,	"11g Transmit Rates"
HKR,NDI\params\TransmitRate11g,type,,		"enum"
HKR,NDI\params\TransmitRate11g,Default,,	"11"

HKR,NDI\params\TransmitRate11g\enum,0,,		"1 Mbps"
HKR,NDI\params\TransmitRate11g\enum,1,,		"2 Mbps"
HKR,NDI\params\TransmitRate11g\enum,2,,		"5.5 Mbps"
HKR,NDI\params\TransmitRate11g\enum,3,,		"11 Mbps"
HKR,NDI\params\TransmitRate11g\enum,4,,		"6 Mbps"
HKR,NDI\params\TransmitRate11g\enum,5,,		"9 Mbps"
HKR,NDI\params\TransmitRate11g\enum,6,,		"12 Mbps"
HKR,NDI\params\TransmitRate11g\enum,7,,		"18 Mbps"
HKR,NDI\params\TransmitRate11g\enum,8,,		"24 Mbps"
HKR,NDI\params\TransmitRate11g\enum,9,,		"36 Mbps"
HKR,NDI\params\TransmitRate11g\enum,10,,	"48 Mbps"
HKR,NDI\params\TransmitRate11g\enum,11,,	"54 Mbps"

[customer0.5213.abg.reg]
HKR, ,                                  NetBand,                        0x00002,  "1823"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1

HKR,NDI\params\TransmitRate11g,ParamDesc,,	"11g Transmit Rates"
HKR,NDI\params\TransmitRate11g,type,,		"enum"
HKR,NDI\params\TransmitRate11g,Default,,	"11"

HKR,NDI\params\TransmitRate11g\enum,0,,		"1 Mbps"
HKR,NDI\params\TransmitRate11g\enum,1,,		"2 Mbps"
HKR,NDI\params\TransmitRate11g\enum,2,,		"5.5 Mbps"
HKR,NDI\params\TransmitRate11g\enum,3,,		"11 Mbps"
HKR,NDI\params\TransmitRate11g\enum,4,,		"6 Mbps"
HKR,NDI\params\TransmitRate11g\enum,5,,		"9 Mbps"
HKR,NDI\params\TransmitRate11g\enum,6,,		"12 Mbps"
HKR,NDI\params\TransmitRate11g\enum,7,,		"18 Mbps"
HKR,NDI\params\TransmitRate11g\enum,8,,		"24 Mbps"
HKR,NDI\params\TransmitRate11g\enum,9,,		"36 Mbps"
HKR,NDI\params\TransmitRate11g\enum,10,,	"48 Mbps"
HKR,NDI\params\TransmitRate11g\enum,11,,	"54 Mbps"

HKR,NDI\params\TransmitRate11a,ParamDesc,,	"11a Transmit Rates"
HKR,NDI\params\TransmitRate11a,type,,		"enum"
HKR,NDI\params\TransmitRate11a,Default,,	"7"

HKR,NDI\params\TransmitRate11a\enum,0,,		"6 Mbps"
HKR,NDI\params\TransmitRate11a\enum,1,,		"9 Mbps"
HKR,NDI\params\TransmitRate11a\enum,2,,		"12 Mbps"
HKR,NDI\params\TransmitRate11a\enum,3,,		"18 Mbps"
HKR,NDI\params\TransmitRate11a\enum,4,,		"24 Mbps"
HKR,NDI\params\TransmitRate11a\enum,5,,		"36 Mbps"
HKR,NDI\params\TransmitRate11a\enum,6,,		"48 Mbps"
HKR,NDI\params\TransmitRate11a\enum,7,,		"54 Mbps"

HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "1823"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "1823",                         0,  "Auto"
HKR, Ndi\params\NetBand\enum,           "1795",                         0,  "5Ghz Only"
HKR, Ndi\params\NetBand\enum,           "28",                           0,  "2.4Ghz Only"

[customer0.5211.reg]
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTimeValidcust%
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          default,                        0,  "45000"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "enum"
HKR, Ndi\params\scanTimeValid\enum,     "120000",                       0,  "120"
HKR, Ndi\params\scanTimeValid\enum,     "60000",                        0,  "60"
HKR, Ndi\params\scanTimeValid\enum,     "45000",                        0,  "45"
HKR, Ndi\params\scanTimeValid\enum,     "30000",                        0,  "30"
HKR, Ndi\params\scanTimeValid\enum,     "20000",                        0,  "20"
HKR, Ndi\params\scanTimeValid\enum,     "10000",                        0,  "10"
HKR, Ndi\params\scanTimeValid\enum,     "5000",                         0,  "5"

HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,  %roamRssiA%
HKR, Ndi\params\roamRssiA,              default,                        0,  "15"
HKR, Ndi\params\roamRssiA,              min,                            0,  "1"
HKR, Ndi\params\roamRssiA,              max,                            0,  "95"
HKR, Ndi\params\roamRssiA,           	step,                           0,  "1"
HKR, Ndi\params\roamRssiA,           	base,                           0,  "10"
HKR, Ndi\params\roamRssiA,           	type,                           0,  "int"

HKR, Ndi\params\NetworkAddress,         ParamDesc,                      0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,         default,                        0,  ""
HKR, Ndi\params\NetworkAddress,         LimitText,                      0,  "12"
HKR, Ndi\params\NetworkAddress,         UpperCase,                      0,  "1"
HKR, Ndi\params\NetworkAddress,         optional,                       0,  "1"
HKR, Ndi\params\NetworkAddress,         type,                           0,  "edit"

HKR, Ndi\params\tpc,                    ParamDesc,                      0,  %tpc%
HKR, Ndi\params\tpc,                    Base,                           0,  "10"
HKR, Ndi\params\tpc,                    default,                        0,  "0"
HKR, Ndi\params\tpc,                    type,                           0,  "enum"
HKR, Ndi\params\tpc\enum,               "0",                            0,  %tpc100%
HKR, Ndi\params\tpc\enum,               "1",                            0,  %tpc50%
HKR, Ndi\params\tpc\enum,               "2",                            0,  %tpc25%
HKR, Ndi\params\tpc\enum,               "3",                            0,  %tpc12%
HKR, Ndi\params\tpc\enum,               "4",                            0,  %tpcLowest%

HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  "1"
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%

;Following Entry made to Enable/Disable rate Auto Rate control.
HKR,NDI\params\rateCtrlEnable,ParamDesc,,	"Auto Transmit Rate"
HKR,NDI\params\rateCtrlEnable,type,,		"enum"
HKR,NDI\params\rateCtrlEnable,Default,,		"1"
HKR,NDI\params\rateCtrlEnable\enum,0,,		"Disable"
HKR,NDI\params\rateCtrlEnable\enum,1,,		"Enable"

;Following Entry made to 11d mode switch 
HKR,NDI\params\ignore11dBeacon,ParamDesc,,	"11d Mode Switch"
HKR,NDI\params\ignore11dBeacon,type,,		"enum"
HKR,NDI\params\ignore11dBeacon,Default,,	"1"
HKR,NDI\params\ignore11dBeacon\enum,0,,		"Enable"
HKR,NDI\params\ignore11dBeacon\enum,1,,		"Disable"

HKR,NDI\params\TransmitRate11b,ParamDesc,,	"11b Transmit Rates"
HKR,NDI\params\TransmitRate11b,type,,		"enum"
HKR,NDI\params\TransmitRate11b,Default,,	"3"

HKR,NDI\params\TransmitRate11b\enum,0,,		"1 Mbps"
HKR,NDI\params\TransmitRate11b\enum,1,,		"2 Mbps"
HKR,NDI\params\TransmitRate11b\enum,2,,		"5.5 Mbps"
HKR,NDI\params\TransmitRate11b\enum,3,,		"11 Mbps"

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,  %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,  "10"
HKR, Ndi\params\radioEnable,            default,                        0,  "1"
HKR, Ndi\params\radioEnable,            type,                           0,  "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,  %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,  %radioEnableOff%

HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR, ,					scanTimePreSleep,               0x00002,  "60" 
HKR, ,					capLinkSp,               	0x00002,  "1" 
HKR, ,                                  abolt,                          0x00002,  "191"

HKR, CustomParams\Configurations,       MajorVersion,                   0x10003,  2
HKR, CustomParams\Configurations,       MinorVersion,                   0x10003,  0

HKR, CustomParams\Configurations,       SelectedConfigurationIndex,     0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationName,      0x00002,  "Default"

[customer0.PS1.reg]
;HKR, CustomParams\Configurations\Cfg0,  PowerManagement,                0x10003,  1 ;Set power Mgmt mode to Max.
HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "1"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

;[customer0.PS2.reg]
;HKR, CustomParams\Configurations\Cfg0,  PowerManagement,                0x10003,  2 ;Set power Mgmt mode to Normal.
;HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
;HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
;HKR, Ndi\params\sleepMode,              default,                        0,  "1"
;HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
;HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
;HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
;HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

[customer0.LED.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "0"

[customer0.LED1.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  pcieClockReq,                   0x00002,  "0"
HKR, ,                                  pciePowerSaveEnable,            0x00002,  "1"
HKR, ,                                  pcieAspm,                       0x00002,  "2"

[customer0.LED2.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  pcieClockReq,                   0x00002,  "0"
HKR, ,                                  pciePowerSaveEnable,            0x00002,  "1"
HKR, ,                                  pcieAspm,                       0x00002,  "2"

[wnaled.reg]
HKR, ,                                  softLEDEnable,                  0x00002,  "1"
HKR, ,                                  swapDefaultLED,                 0x00002,  "1"

[customer1ani.reg]
HKR, Ndi\params\rssiThrHigh,            ParamDesc,                      0,        %rssiThrHigh%
HKR, Ndi\params\rssiThrHigh,            Base,                           0,        "10"
HKR, Ndi\params\rssiThrHigh,            default,                        0,        "40"
HKR, Ndi\params\rssiThrHigh,            type,                           0,        "enum"
HKR, Ndi\params\rssiThrHigh\enum,       "40",                           0,        %rssiThrHighNormal%
HKR, Ndi\params\rssiThrHigh\enum,       "32",                           0,        %rssiThrHighMin%

[customer3.reg]
HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "1"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%
HKR, ,                                  scanTimePreSleep,		0x00002,  "60"
HKR, ,                                  SleepTimePerf,			0x00002,  "500"
HKR, ,                                  LinkLEDFunc,			0x00002,  "19"
HKR, ,                                  ActivityLEDFunc,		0x00002,  "21"

[customer3a.reg]
HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "1"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  pciePowerSaveEnable,            0x00002,  "1"
HKR, ,                                  pcieClockReq,                   0x00002,  "0"
HKR, ,                                  pcieAspm,                       0x00002,  "0"
HKR, ,                                  abolt,                          0x00002,  "0"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "0"

[customer1a3b.reg]
HKR, ,                                  NetBand,                        0x00002,  "61455"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, ,                                  rmEnable,                       0x00002,  "1"
HKR, ,                                  abolt,                          0x00002,  "0"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                          	gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[customer4a.reg]
HKR, ,					gpioPinFunc0,        		0x00002,  "1"
HKR, ,					gpioFunc0ActHi,      		0x00002,  "0"
HKR, ,					PcieClockReq,     		0x00002,  "0"

[customer4b.reg]
HKR, ,					gpioPinFunc0,        		0x00002,  "3"
HKR, ,					gpioFunc0ActHi,      		0x00002,  "0"
HKR, ,					PcieClockReq,     		0x00002,  "0"

[customer4_basic.reg]
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"
HKR, ,                                  abolt,                          0x00002,  "0"
HKR, ,                                  sleepMode,                      0x00002, %sleepMode_DEFAULT%
HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  %sleepMode_DEFAULT%
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%
HKR, ,                                  shortPreamble,                  0x00002, %shortPreamble_DEFAULT%
HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  %shortPreamble_DEFAULT%
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%
HKR, Ndi\params\authTypeUseOnly,        ParamDesc,                      0,  %authTypeUseOnly%
HKR, Ndi\params\authTypeUseOnly,        Base,                           0,  "10"
HKR, Ndi\params\authTypeUseOnly,        default,                        0,  "0"
HKR, Ndi\params\authTypeUseOnly,        type,                           0,  "enum"
HKR, Ndi\params\authTypeUseOnly\enum,   "0",                            0,  %authAuto%
HKR, Ndi\params\authTypeUseOnly\enum,   "1",                            0,  %authOpen%
HKR, Ndi\params\authTypeUseOnly\enum,   "2",                            0,  %authShared%
HKR, ,                                  beaconInterval,                 0x00002,  "100"
HKR, ,                                  bkScanEnable,                   0x00002,  "1"
HKR, ,                                  bssType,                        0x00002,  "1"
HKR, ,                                  ccode,                          0x00002,  "US"
HKR, ,                                  clist,                          0x00002,  ""
HKR, ,                                  defaultKey,                     0x00002,  "0"
HKR, ,                                  EncryptionAlg,                  0x00002,  "2"
HKR, ,                                  FragThreshold,                  0x00002,  "2346"
HKR, ,                                  HwTxRetries,                    0x00002,  "4"
HKR, ,                                  privacyInvoked,                 0x00002,  "0"
HKR, ,                                  QoS,                            0x00002,  "0"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                                  RTSThreshold,                   0x00002,  "2346"
HKR, ,                                  scanType,                       0x00002,  "2"
HKR, ,                                  SwTxRetryScale,                 0x00002,  "6"
HKR, ,                                  SmeEnable,                      0x00002,  "1"
HKR, ,                                  adhocChannel,                   0x00002,  "2462"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  capLinkSp,                      0x00002,  "2"
HKR, ,                                  pcieAspm,                       0x00002,  "0"
HKR, ,                                  LanExpress,                     0,         "AS00"
HKR, ,                                  DynamicConfig,                  0,         "0"

[customer4a_ASPM.reg]
HKR, ,                                  pcieAspm,                       0x00002,  "0"

[customer5.reg]
HKR, ,                                  forceBias,                      0x00002,  "2"
HKR, ,                                  enable2GHzHt40Cap,                    0,  "1"

[customer5.11nLED.reg]
HKR, ,                                  gpioLedCustom,                  0x00002,  "1"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "2"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "1"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "0"

[customer5.3x3.reg]
HKR, ,                                  txChainSelect,                 	0x00002,  "7"
HKR, ,                                  RxChainSelect,                 	0x00002,  "7"

[customer5.PCIe11nLed.reg]
HKR, ,                                  gpioLedCustom,                  0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"

[customer6Led.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[customer9.reg]
HKR, Ndi\params\MapRegisters,           ParamDesc,                      0,  %MapRegisters%
HKR, Ndi\params\MapRegisters,           default,                        0,  "256"
HKR, Ndi\params\MapRegisters,           min,                            0,  "32"
HKR, Ndi\params\MapRegisters,           max,                            0,  "512"
HKR, Ndi\params\MapRegisters,           step,                           0,  "8"
HKR, Ndi\params\MapRegisters,           base,                           0,  "10"
HKR, Ndi\params\MapRegisters,           type,                           0,  "int"
HKR, Ndi\params\NetworkAddress,         ParamDesc,                      0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,         default,                        0,  ""
HKR, Ndi\params\NetworkAddress,         LimitText,                      0,  "12"
HKR, Ndi\params\NetworkAddress,         UpperCase,                      0,  "1"
HKR, Ndi\params\NetworkAddress,         optional,                       0,  "1"
HKR, Ndi\params\NetworkAddress,         type,                           0,  "edit"
HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "2"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%
HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  "1"
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%
HKR, Ndi\params\radioEnable,            ParamDesc,                      0,  %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,  "10"
HKR, Ndi\params\radioEnable,            default,                        0,  "1"
HKR, Ndi\params\radioEnable,            type,                           0,  "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,  %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,  %radioEnableOff%
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"
HKR, Ndi\params\ccx5FeatureEnable,      ParamDesc,                      0,  %ccx5FeatureEnable%
HKR, Ndi\params\ccx5FeatureEnable,      Base,                           0,  "10"
HKR, Ndi\params\ccx5FeatureEnable,      default,                        0,  "0"
HKR, Ndi\params\ccx5FeatureEnable,      type,                           0,  "enum"
HKR, Ndi\params\ccx5FeatureEnable\enum, "1",                            0,  %ccx5FeatureEnableMfpEnable%
HKR, Ndi\params\ccx5FeatureEnable\enum, "0",                            0,  %ccx5FeatureEnableMfpDisable%
HKR, CustomParams\Configurations,       MajorVersion,                   0x10003,  2
HKR, CustomParams\Configurations,       MinorVersion,                   0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationIndex,     0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationName,      0x00002,  "Default"
HKR, ,                                  AwakeTimePerf,                  0,  "1000"                  
HKR, ,                                  abolt,                          0x00002,  "0"
HKR, ,                                  pcieAspm,                       0x00002,  "0"

[COMMON_AG.reg]
HKR, ,                                  NetBand,                        0x00002,  %NetBand_DEF_STR_AG%
HKR, ,                                  AdHocBand,                      0x00002,  %AdhocBand_DEF_STR_AG%
HKR, CustomParams\Configurations,       NicType,                        0x10003,  2

[10261a3b.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,									OemLinkLED,			    		0x00002,  "1"

[customer10.LED3.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"

[customer10.reg]
HKR, ,                                  gpioPinFunc1,                  0x00002,  "1"

[customer11.reg]
HKR, Ndi\params\MapRegisters,           ParamDesc,                      0,  %MapRegisters%
HKR, Ndi\params\MapRegisters,           default,                        0,  "256"
HKR, Ndi\params\MapRegisters,           min,                            0,  "32"
HKR, Ndi\params\MapRegisters,           max,                            0,  "512"
HKR, Ndi\params\MapRegisters,           step,                           0,  "8"
HKR, Ndi\params\MapRegisters,           base,                           0,  "10"
HKR, Ndi\params\MapRegisters,           type,                           0,  "int"

HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "2"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  "1"
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,  %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,  "10"
HKR, Ndi\params\radioEnable,            default,                        0,  "1"
HKR, Ndi\params\radioEnable,            type,                           0,  "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,  %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,  %radioEnableOff%

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"

HKR, Ndi\params\ccx5FeatureEnable,      ParamDesc,                      0,  %ccx5FeatureEnable%
HKR, Ndi\params\ccx5FeatureEnable,      Base,                           0,  "10"
HKR, Ndi\params\ccx5FeatureEnable,      default,                        0,  "0"
HKR, Ndi\params\ccx5FeatureEnable,      type,                           0,  "enum"
HKR, Ndi\params\ccx5FeatureEnable\enum, "1",                            0,  %ccx5FeatureEnableMfpEnable%
HKR, Ndi\params\ccx5FeatureEnable\enum, "0",                            0,  %ccx5FeatureEnableMfpDisable%

HKR, CustomParams\Configurations,       MajorVersion,                   0x10003,  2
HKR, CustomParams\Configurations,       MinorVersion,                   0x10003,  0

HKR, CustomParams\Configurations,       SelectedConfigurationIndex,     0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationName,      0x00002,  "Default"

HKR, CustomParams\Configurations,       NicType,                        0x10003,  1

HKR, Ndi\params\bkScanEnable,           ParamDesc,                      0,        %bkScanEnable%
HKR, Ndi\params\bkScanEnable,           Base,                           0,        "10"
HKR, Ndi\params\bkScanEnable,           default,                        0,        "1"
HKR, Ndi\params\bkScanEnable,           type,                           0,        "enum"
HKR, Ndi\params\bkScanEnable\enum,      "1",                            0,        %bkScanEnableOn%
HKR, Ndi\params\bkScanEnable\enum,      "0",                            0,        %bkScanEnableOff%

HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,        %roamRssi11A%
HKR, Ndi\params\roamRssiA,              default,                        0,        "15"
HKR, Ndi\params\roamRssiA,              min,                            0,        "1"
HKR, Ndi\params\roamRssiA,              max,                            0,        "95"
HKR, Ndi\params\roamRssiA,              step,                           0,        "1"
HKR, Ndi\params\roamRssiA,              base,                           0,        "10"
HKR, Ndi\params\roamRssiA,              type,                           0,        "int"

HKR, Ndi\params\roamRssiBOnly,          ParamDesc,                      0,        %roamRssi11BOnly%
HKR, Ndi\params\roamRssiBOnly,          default,                        0,        "8"
HKR, Ndi\params\roamRssiBOnly,          min,                            0,        "0"
HKR, Ndi\params\roamRssiBOnly,          max,                            0,        "95"
HKR, Ndi\params\roamRssiBOnly,          step,                           0,        "1"
HKR, Ndi\params\roamRssiBOnly,          base,                           0,        "10"
HKR, Ndi\params\roamRssiBOnly,          type,                           0,        "int"

HKR, Ndi\params\roamRssiB,              ParamDesc,                      0,        %roamRssi11B%
HKR, Ndi\params\roamRssiB,              default,                        0,        "24"
HKR, Ndi\params\roamRssiB,              min,                            0,        "0"
HKR, Ndi\params\roamRssiB,              max,                            0,        "95"
HKR, Ndi\params\roamRssiB,              step,                           0,        "1"
HKR, Ndi\params\roamRssiB,              base,                           0,        "10"
HKR, Ndi\params\roamRssiB,              type,                           0,        "int"

HKR, Ndi\params\roamRateA,              ParamDesc,                      0,        %roamRateA%
HKR, Ndi\params\roamRateA,              Base,                           0,        "10"
HKR, Ndi\params\roamRateA,              default,                        0,        "24000"
HKR, Ndi\params\roamRateA,              type,                           0,        "enum"
HKR, Ndi\params\roamRateA\enum,         "6000",                         0,        %roamRateA6M%
HKR, Ndi\params\roamRateA\enum,         "9000",                         0,        %roamRateA9M%
HKR, Ndi\params\roamRateA\enum,         "12000",                        0,        %roamRateA12M%
HKR, Ndi\params\roamRateA\enum,         "18000",                        0,        %roamRateA18M%
HKR, Ndi\params\roamRateA\enum,         "24000",                        0,        %roamRateA24M%
HKR, Ndi\params\roamRateA\enum,         "36000",                        0,        %roamRateA36M%
HKR, Ndi\params\roamRateA\enum,         "48000",                        0,        %roamRateA48M%
HKR, Ndi\params\roamRateA\enum,         "54000",                        0,        %roamRateA54M%

HKR, Ndi\params\roamRateBOnly,          ParamDesc,                      0,        %roamRateBOnly%
HKR, Ndi\params\roamRateBOnly,          Base,                           0,        "10"
HKR, Ndi\params\roamRateBOnly,          default,                        0,        "5000"
HKR, Ndi\params\roamRateBOnly,          type,                           0,        "enum"
HKR, Ndi\params\roamRateBOnly\enum,     "1000",                         0,        %roamRateBOnly1M%
HKR, Ndi\params\roamRateBOnly\enum,     "2000",                         0,        %roamRateBOnly2M%
HKR, Ndi\params\roamRateBOnly\enum,     "5000",                         0,        %roamRateBOnly5M%
HKR, Ndi\params\roamRateBOnly\enum,     "11000",                        0,        %roamRateBOnly11M%

HKR, Ndi\params\roamRateB,              ParamDesc,                      0,        %roamRateB%
HKR, Ndi\params\roamRateB,              Base,                           0,        "10"
HKR, Ndi\params\roamRateB,              default,                        0,        "9000"
HKR, Ndi\params\roamRateB,              type,                           0,        "enum"
HKR, Ndi\params\roamRateB\enum,         "1000",                         0,        %roamRateB1M%
HKR, Ndi\params\roamRateB\enum,         "2000",                         0,        %roamRateB2M%
HKR, Ndi\params\roamRateB\enum,         "5000",                         0,        %roamRateB5M%
HKR, Ndi\params\roamRateB\enum,         "6000",                         0,        %roamRateB6M%
HKR, Ndi\params\roamRateB\enum,         "9000",                         0,        %roamRateB9M%
HKR, Ndi\params\roamRateB\enum,         "11000",                        0,        %roamRateB11M%

HKR, Ndi\params\pcieAspm,               ParamDesc,                      0,        %pcieAspm%
HKR, Ndi\params\pcieAspm,               Base,                           0,        "10"
HKR, Ndi\params\pcieAspm,               default,                        0,        "0"
HKR, Ndi\params\pcieAspm,               type,                           0,        "enum"
HKR, Ndi\params\pcieAspm\enum,          "0",                            0,        %pcieAspmOff%
HKR, Ndi\params\pcieAspm\enum,          "2",                            0,        %pcieAspmL1On%

[customer11_11n40wmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "61467"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "40964",                        0,        %wModeSelect11bonly%
HKR, Ndi\params\wModeSelect\enum,       "20483",                        0,        %wModeSelect11na%
HKR, Ndi\params\wModeSelect\enum,       "40988",                        0,        %wModeSelect11nbg%
HKR, Ndi\params\wModeSelect\enum,       "61467",                        0,        %wModeSelect11abgn%

[customer11_11nwmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "49719"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "32772",                        0,        %wModeSelect11bonly%
HKR, Ndi\params\wModeSelect\enum,       "16387",                        0,        %wModeSelect11na%
HKR, Ndi\params\wModeSelect\enum,       "32796",                        0,        %wModeSelect11nbg%
HKR, Ndi\params\wModeSelect\enum,       "49719",                        0,        %wModeSelect11abgn%

[customer11_legacywmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "2075"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "4",                            0,        %wModeLegacy11bonly%
HKR, Ndi\params\wModeSelect\enum,       "3",                            0,        %wModeLegacy11a%
HKR, Ndi\params\wModeSelect\enum,       "28",                           0,        %wModeLegacy11bg%
HKR, Ndi\params\wModeSelect\enum,       "2075",                         0,        %wModeLegacy11abg%

[customer11Ant.reg]
HKR, Ndi\params\antennaSwitch,          ParamDesc,                      0,        %antennaSwitch%
HKR, Ndi\params\antennaSwitch,          Base,                           0,        "10"
HKR, Ndi\params\antennaSwitch,          default,                        0,        "0"
HKR, Ndi\params\antennaSwitch,          type,                           0,        "enum"
HKR, Ndi\params\antennaSwitch\enum,     "1",                            0,        %antennaSwitchA%
HKR, Ndi\params\antennaSwitch\enum,     "2",                            0,        %antennaSwitchB%
HKR, Ndi\params\antennaSwitch\enum,     "0",                            0,        %antennaSwitchAuto%

[customer11Led.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[customer11ACStatus.reg]
HKR, ,                                  overrideACstatus,               0x00002,  "2"

[customer12.reg]
HKR, ,                                  txChainSelect,                 	0x00002,  "5"

[customer12Led0.reg]
HKR, ,                  		LinkLedFunc,       		0, "19"
HKR, ,                  	        ActivityLedFunc,       	        0, "21" 

[customer12Led1.reg]
HKR, ,                  		LinkLedFunc,       		0, "03"
HKR, ,                  		ActivityLedFunc,       		0, "05"

[customer12led2.reg]
HKR, ,                  		LinkLedFunc,       		0, "07"
HKR, ,                  		ActivityLedFunc,       		0, "05"

[Customer14.led.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[customer_Samsung.reg]
HKR,NDI\params\ignore11dBeacon,ParamDesc,,	"802.11d"
HKR,NDI\params\ignore11dBeacon,type,,		"enum"
HKR,NDI\params\ignore11dBeacon,Default,,	"1"
HKR,NDI\params\ignore11dBeacon\enum,0,,		"Enable"
HKR,NDI\params\ignore11dBeacon\enum,1,,		"Disable"
HKR, Ndi\params\NetBand,                ParamDesc,                      0,        %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,        "10"
HKR, Ndi\params\NetBand,                default,                        0,        "28"
HKR, Ndi\params\NetBand,                type,                           0,        "enum"
HKR, Ndi\params\NetBand\enum,           "28",                           0,        "802.11b+g"
HKR, Ndi\params\NetBand\enum,           "4",                            0,        "802.11b"
HKR, ,                                  overrideACstatus,               0x00002,  "1"

[rssiAdjust.reg]
HKR, ,                                  rssiAdjust,                     0x00002,  "7"

;-----------------------------------------------------------------------------
; ATHER NT specific
;

[ATHER.reg]
HKR, Ndi,             Service,      0, "AR5416"
HKR, Ndi\Interfaces,  UpperRange,   0, "ndis5"
HKR, Ndi\Interfaces,  LowerRange,   0, "ethernet"

[ATHER.Service]
DisplayName     = %ATHER.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\athw.sys
LoadOrderGroup  = NDIS

;-----------------------------------------------------------------------------
; ATHER NT/XP common
;
[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, ,                  EventMessageFile,   0x00020000,   "%%SystemRoot%%\System32\netevent.dll"
HKR, ,                  TypesSupported,     0x00010001,   7

;----------------------------------------------------------------------------
; Remark whole Win9x Section since Win98/Win98se/WinMe is no longer supported
; This section to be deleted
; ATHER Win9x specific
;
;[ATHER.win.reg]
;HKR, ,                  DevLoader,          0,            "*ndis"
;HKR, ,                  DeviceVxDs,         0,            "ar54169x.sys"
;HKR, ,                  EnumPropPages,      0,            "netdi.dll,EnumPropPages"

;HKR, Ndi\Interfaces,    DefUpper,           0,            "ndis3"
;HKR, Ndi\Interfaces,    DefLower,           0,            "ethernet"
;HKR, Ndi\Interfaces,    UpperRange,         0,            "ndis3"
;HKR, Ndi\Interfaces,    LowerRange,         0,            "ethernet"


;HKR, NDIS,              LogDriverName,      0,            "AR54169X"
;HKR, NDIS,              MajorNdisVersion,   1,            03
;HKR, NDIS,              MinorNdisVersion,   1,            0A

;HKR, Ndi\Install,       ndis3,              0,            "ATHER.install"

;----------------------------------------------------------------------------
; System TCPIP parameter changes
;
[sys.TcpParams.reg]
HKLM, SYSTEM\CurrentControlSet\Services\Tcpip\Parameters, Tcp1323Opts, 0x00010001, 0x00000003
HKLM, SYSTEM\CurrentControlSet\Services\Tcpip\Parameters, TcpWindowSize, 0x00010001, 0x00040000

;----------------------------------------------------------------------------
; Remark whole Win9x Section since Win98/Win98se/WinMe is no longer supported
; This section to be deleted
; Win9x Files to Copy
;[ATHER.win.CopyFiles]
;ar54169x.sys,,,2

;----------------------------------------------------------------------------
; NT Files to Copy
[ATHER.CopyFiles.nt]
athw.sys,,,2

[ATHER.DelIniFiles]
Athnic.ini,,,1

[SourceDisksNames]
;
; diskid = description[, [tagfile] [, <unused>, subdir]]
;
1 = %Atheros_Disk%,,,

;----------------------------------------------------------------------------
; Source Files
[SourceDisksFiles]
ar54169x.sys                 = 1,, ; on distribution disk 1
athw.sys                   = 1,, ; on distribution disk 1


[DestinationDirs]
ATHER.CopyFiles.nt           = 12
;ATHER.win.CopyFiles          = 10,system32\drivers ; %SystemRoot%\system32\drivers
ATHER.DelIniFiles            = 10,system32\drivers ; %SystemRoot%\system32\drivers
DefaultDestDir               = 11

[DEFAULTDESTDIRS]
;


[Strings]
Atheros                      = "Atheros"
Gigabyte                     = "Gigabyte Technology Corp."			 
MapRegisters                 = "Map Registers"
NetworkAddress               = "Network Address"
sleepMode                    = "Power Save Mode"
scanTimeValid                = "Scan Valid Interval"
scanTime                     = "Roam Time (sec)"
roamRssiA                    = "Roam Time Threshold (db)"
sleepModeOff                 = "Off"
sleepModeNormal              = "Normal"
sleepModeMax                 = "Maximum"
tpc                          = "Transmit Power"
tpcLowest                    = "Lowest"
tpc12                        = "12.5%"
tpc25                        = "25%"
tpc50                        = "50%"
tpc100                       = "100%"
shortPreamble                = "802.11b Preamble"
shortPreambleEnable          = "Long and Short"
shortPreambleDisable         = "Long only"
radioEnable                  = "Radio On/Off"
radioEnableOn                = "On"
radioEnableOff               = "Off"
WirelessMode         	     = "Wireless Mode Selection"
rssiThrHigh                  = "RSSI Threshold"
rssiThrHighNormal            = "Normal"
rssiThrHighMin               = "Min"
scanTimeValidcust            = "Roam Time (sec)"
sleepMode_DEFAULT          = "2"  
NetBand_DEF_STR_A          = "3"                       ; (A/T) 
NetBand_DEF_STR_AB         = "7"                       ; (A/T/B)   
NetBand_DEF_STR_G          = "12"                      ; (B/G)     
NetBand_DEF_STR_AG         = "15"                      ; (A/T/B/G)
AdhocBand_DEF_STR_A        = "1"                       ; (A)
AdhocBand_DEF_STR_AB       = "1"                       ; (A)
AdhocBand_DEF_STR_G        = "0"                       ; (B)
AdhocBand_DEF_STR_AG       = "0"                       ; (B)
shortPreamble_DEFAULT       = "1"
authTypeUseOnly              = "802.11 Authentication Type"
authAuto                     = "Auto"
authOpen                     = "Open"
authShared                   = "Shared"
bkScanEnable                 = "BackgroundScan On/Off"
bkScanEnableOn               = "On"
bkScanEnableOff              = "Off"
roamRssi11A                  = "roamRssiA"
roamRssi11B                  = "roamRssiB"
roamRssi11BOnly              = "roamRssiBOnly"
roamRateA                    = "roamRateA"
roamRateA6M                  = " 6Mbps"
roamRateA9M                  = " 9Mbps"
roamRateA12M                 = "12Mbps"
roamRateA18M                 = "18Mbps"
roamRateA24M                 = "24Mbps"
roamRateA36M                 = "36Mbps"
roamRateA48M                 = "48Mbps"
roamRateA54M                 = "54Mbps"
roamRateBOnly                = "roamRateBOnly"
roamRateBOnly1M              = " 1Mbps"
roamRateBOnly2M              = " 2Mbps"
roamRateBOnly5M              = " 5Mbps"
roamRateBOnly11M             = "11Mbps"
roamRateB                    = "roamRateB"
roamRateB1M                  = " 1Mbps"
roamRateB2M                  = " 2Mbps"
roamRateB5M                  = " 5Mbps"
roamRateB6M                  = " 6Mbps"
roamRateB9M                  = " 9Mbps"
roamRateB11M                 = "11Mbps"
pcieAspm                     = "pcieAspm"
pcieAspmOff                  = "L0s Off, L1 Off"
pcieAspmL1On                 = "L0s Off, L1 On"
wModeSelect                  = "Wireless Mode"
wModeSelect11bonly           = "11b only"
wModeSelect11nbg             = "11n(2.4GHz) and g and b"
wModeSelect11na              = "11n(5GHz) and a"
wModeSelect11abgn            = "11abgn"
wModeLegacy11a               = "11a only"
wModeLegacy11bonly           = "11b only"
wModeLegacy11bg              = "11g and 11b"
wModeLegacy11abg             = "11abg"
antennaSwitch                = "AntennaSwitch"
antennaSwitchAuto            = "Auto"
antennaSwitchA               = "Antenna A"
antennaSwitchB               = "Antenna B"
uapsdEnabledBE               = "Power Save Policy (Best Effort)"
uapsdEnabledBEOn             = "WMM Power Save (UAPSD)"
uapsdEnabledBEOff            = "Legacy Power Save"
uapsdEnabledBK               = "Power Save Policy (Background)"
uapsdEnabledBKOn             = "WMM Power Save (UAPSD)"
uapsdEnabledBKOff            = "Legacy Power Save"
uapsdEnabledVI               = "Power Save Policy (Voice)"
uapsdEnabledVIOn             = "WMM Power Save (UAPSD)"
uapsdEnabledVIOff            = "Legacy Power Save"
uapsdEnabledVO               = "Power Save Policy (Video)"
uapsdEnabledVOOn             = "WMM Power Save (UAPSD)"
uapsdEnabledVOOff            = "Legacy Power Save"
ccx5FeatureEnable            = "MFP"
ccx5FeatureEnableMfpEnable   = "Enable"
ccx5FeatureEnableMfpDisable  = "Disable"

Atheros_Disk                 = "Atheros Driver Disk 1"
ATHER.Service.DispName       = "Atheros AR5008 Wireless Network Adapter Service"
ATHER.DeviceDesc.0013        = "Atheros Wireless Network Adapter"
ATHER.DeviceDesc.001A        = "Atheros AR5005G Wireless Network Adapter"
ATHER.DeviceDesc.001B        = "Atheros AR5006X Wireless Network Adapter"
ATHER.DeviceDesc.1025        = "Atheros AR5001X+ Wireless Network Adapter"
ATHER.DeviceDesc.2025        = "Atheros AR5001X+ Wireless Network Adapter"
ATHER.DeviceDesc.1026        = "Atheros AR5001X+ Wireless Network Adapter"
ATHER.DeviceDesc.2026        = "Atheros AR5001X+ Wireless Network Adapter"
ATHER.DeviceDesc.1027        = "Atheros AR5001X+ Wireless Network Adapter"
ATHER.DeviceDesc.2027        = "Atheros AR5001X+ Wireless Network Adapter"
ATHER.DeviceDesc.1030        = "Atheros AR5002G Wireless Network Adapter"
ATHER.DeviceDesc.2030        = "Atheros AR5002G Wireless Network Adapter"
ATHER.DeviceDesc.1031        = "Atheros AR5002X Wireless Network Adapter"
ATHER.DeviceDesc.2031        = "Atheros AR5002X Wireless Network Adapter"
ATHER.DeviceDesc.1041        = "Atheros AR5004G Wireless Network Adapter"
ATHER.DeviceDesc.2041        = "Atheros AR5004G Wireless Network Adapter"
ATHER.DeviceDesc.1042        = "Atheros AR5004X Wireless Network Adapter"
ATHER.DeviceDesc.2042        = "Atheros AR5004X Wireless Network Adapter"
ATHER.DeviceDesc.1051        = "Atheros AR5005GS Wireless Network Adapter"
ATHER.DeviceDesc.2051        = "Atheros AR5005GS Wireless Network Adapter"
ATHER.DeviceDesc.1053        = "Atheros AR5005GS Wireless Network Adapter"
ATHER.DeviceDesc.2053        = "Atheros AR5005GS Wireless Network Adapter"
ATHER.DeviceDesc.1062        = "Atheros AR5006XS Wireless Network Adapter"
ATHER.DeviceDesc.2062        = "Atheros AR5006XS Wireless Network Adapter"
ATHER.DeviceDesc.3062        = "Atheros AR5006EXS Wireless Network Adapter"
ATHER.DeviceDesc.3063        = "Atheros AR5006EX Wireless Network Adapter"
ATHER.DeviceDesc.3061        = "Atheros AR5006EGS Wireless Network Adapter"
ATHER.DeviceDesc.3065        = "Atheros AR5006EG Wireless Network Adapter"
ATHER.DeviceDesc.2061        = "Atheros AR5006GS Wireless Network Adapter"
ATHER.DeviceDesc.1061        = "Atheros AR5006GS Wireless Network Adapter"
ATHER.DeviceDesc.2065        = "Atheros AR5006G Wireless Network Adapter"
ATHER.DeviceDesc.1065        = "Atheros AR5006G Wireless Network Adapter"
ATHER.DeviceDesc.0055        = "IEEE 802.11a/g Wireless LAN Adapter (A)"
ATHER.DeviceDesc.10CF        = "IEEE 802.11a/g Wireless LAN Adapter (A)"
ATHER.DeviceDesc.3067        = "Atheros AR5007EG Wireless Network Adapter"
ATHER.DeviceDesc.001D        = "Atheros AR5007G Wireless Network Adapter"
ATHER.DeviceDesc.1055        = "Atheros AR5007G Wireless Network Adapter"
ATHER.DeviceDesc.2055        = "Atheros AR5007G Wireless Network Adapter"
ATHER.DeviceDesc.3013        = "11b/g Wireless LAN Mini PCI Express Adapter"
ATHER.DeviceDesc.4013        = "11a/b/g Wireless LAN Mini PCI Express Adapter" 
ATHER.DeviceDesc.1013        = "11b/g Wireless LAN Mini PCI Adapter"
ATHER.DeviceDesc.2013        = "11a/b/g Wireless LAN Mini PCI Adapter II" 
ATHER.DeviceDesc.5013        = "11b/g Wireless LAN Mini PCI Express Adapter II"  
ATHER.DeviceDesc.6013        = "11b/g Wireless LAN Mini PCI Express Adapter III"  
ATHER.DeviceDesc.0023        = "Atheros AR5008 Wireless Network Adapter"
ATHER.DeviceDesc.0032168c    = "11b/g/n Wireless LAN Mini-PCI Express Adapter"
ATHER.DeviceDesc.0033168c    = "11a/b/g/n Wireless LAN Mini-PCI Express Adapter"
ATHER.DeviceDesc.E000        = "LAN-Express AS IEEE 802.11g PCI-E Adapter"
ATHER.DeviceDesc.0406        = "LAN-Express AS IEEE 802.11g miniPCI Adapter" 
ATHER.DeviceDesc.0407        = "LAN-Express AS IEEE 802.11a/g miniPCI Adapter"
ATHER.DeviceDesc.3072        = "Atheros AR5008X Wireless Network Adapter"
GIGA.DeviceDesc.E914	     = "Gigabyte GN-WI03N (mini) PCI WLAN Card"
GIGA.DeviceDesc.E915	     = "Gigabyte GN-WP02N PCI Express WLAN Card"
GIGA.DeviceDesc.E916	     = "Gigabyte GN-WI06N (mini) PCI Express WLAN Card"
GIGA.DeviceDesc.E815	     = "Gigabyte GN-WM02N Express WLAN Card"
GIGA.DeviceDesc.E801         = "Gigabyte GN-WLMA102 Cardbus WLAN Card"
GIGA.DeviceDesc.E811         = "Gigabyte GN-WMAG Cardbus WLAN Card"
GIGA.DeviceDesc.E814         = "Gigabyte GN-WM01GT Cardbus WLAN Card"
GIGA.DeviceDesc.0013         = "Gigabyte GN-WIAH (mini) PCI WLAN Card"
GIGA.DeviceDesc.E901         = "Gigabyte GN-WI01HT (mini) PCI WLAN Card"
GIGA.DeviceDesc.E911         = "Gigabyte GN-WIAG/GN-WPEAG (mini) PCI WLAN Card"
GIGA.DeviceDesc.E912         = "Gigabyte GN-WP01GT (mini) PCI WLAN Card"
GIGA.DeviceDesc.E913         = "Gigabyte GN-WI01GT (mini) PCI-E WLAN Card"
GIGA.DeviceDesc.E917         = "Gigabyte GN-WI07HT (mini) PCI-E WLAN Card"
GIGA.DeviceDesc.E918        = "Gigabyte GN-WS50G (mini) PCI-E WLAN Card"
ATHER.DeviceDesc.DWA642      = "D-Link DWA-642 RangeBooster N Notebook Adapter"
ATHER.DeviceDesc.DWA645      = "D-Link DWA-645 RangeBooster N650 Notebook Adapter"
ATHER.DeviceDesc.DWA542      = "D-Link DWA-542 RangeBooster N Desktop Adapter"
ATHER.DeviceDesc.DWA547      = "D-Link DWA-547 RangeBooster N650 Desktop Adapter"
ATHER.DeviceDesc.DWA652      = "D-Link DWA-652 XtremeN Notebook Adapter"
ATHER.DeviceDesc.DWA552      = "D-Link DWA-552 XtremeN Desktop Adapter"
ATHER.DeviceDesc.DWA643      = "D-Link DWA-643 Xtreme N ExpressCard Notebook Adapter"
ATHER.DeviceDesc.DWA556      = "D-Link DWA-556 Xtreme N PCIe Desktop Adapter"
ATHER.DeviceDesc.DWA520      = "D-Link DWA-520 Wireless 108G Desktop Adapter"
ATHER.DeviceDesc.DWA620	     = "D-Link DWA-620 Wireless 108G Notebook Adapter"
ATHER.DeviceDesc.WDA1320     = "D-Link WDA-1320 Wireless G Desktop Adapter"
ATHER.DeviceDesc.WDA2320     = "D-Link WDA-2320 RangeBooster G Desktop Adapter"
ATHER.DeviceDesc.WNA2330     = "D-Link WNA-2330 RangeBooster G Notebook Adapter"
ATHER.DeviceDesc.WNA1330     = "D-Link WNA-1330 Wireless G Notebook Adapter"
ATIWC.DeviceDesc.ATICB	     = "Allied Telesyn AT-WCC201g Wireless Card Bus Adapter"
ATIWC.DeviceDesc.ATIPC	     = "Allied Telesyn AT-WCP201g Wireless PCI Adapter"
ATHER.DeviceDesc.0024	     = "Atheros AR5008X Wireless Network Adapter"