----------------------------------------------------------------------------
                    Install method of NXPAD Driver
----------------------------------------------------------------------------

Please install this driver by the following method.
This method assumes the following composition. 

*Please make sure that you are logged on as administrator when you install this driver.

1. Close all Applications. 

2. Move the mouse pointer to the upper right to display charm bar.

3. Click"Search".

4. Type "cmd" and select the "Command Prompt" shown below.

5. Input"D:\NXPADE\Setup.exe"in command Prompt.
   *If the confirmation screen of the user account control is displayed, click "Yes"

6. "ELAN Input Device Driver Installation"starts,"Welcome"showed and click"Next".

7. After the window "Review the terms of the license agreement"showed, 
   select"I accept this agreement"and click"next".

8. Click "Finish" of "Setup complete".

9. "You must restart your computer to apply these changes" showed, and click"Restart Now".

10. Restart the system.

----------------------------------------------------------------------------
              The check method of NXPAD Driver version
----------------------------------------------------------------------------

1. Move the mouse pointer to the upper right.
 
2. Select"Settings".

3. Choose"Control Panel".
   *the installation check procedure are described by assuming that 
    the View by on the control panel is in the "Category".

4. Click "Hardware and Sound" -> "Devices and Printers" -> "Device Manager" 
   *If the confirmation screen of the user account control is displayed, click "Yes"

5. Double click"Mice and other pointing devices" -> Double click "NX PAD" .

6. Select the "Driver" tab, and check the Driver Version is "11.16.14.1".


This is the End of the way to setup "NXPAD Driver".
