[ Core Center ]   : MSI hardware monitor & overclock & fan control Tool           

Support list : 
	MS-6570E,MS-6580(v5.0),MS-6585(v5.0),MS-6590(v2.0),
	MS-6702(v1.0,v2.0),MS-6702E,MS-6714(v5.0),MS-6728(v1.0,v2.0,v3.0),MS-6741,MS-6758(v1.0,v2.0),MS-6788(v1.0,v2.0),MS-6799,
        MS-7003,MS-7008,MS-7021,MS-7025,MS-7028(v1.0,v2.0),MS-7030,MS-7031,MS-7032,MS-7033,MS-7037,MS-7043,MS-7047,MS-7052,MS-7053,MS-7058,MS-7066,MS-7088,
	MS-7100,MS-7125(v1.0,v3.0,v3.0A),MS-7133,MS-7135,MS-7143(v2X),MS-7151,MS-7157,MS-7158,MS-7160,MS-7166,MS-7175,MS-7176(v1.0,v2.0),MS-7185,MS-7194
	MS-7203,MS-7220,MS-7226,MS-7235,MS-7236,MS-7246,MS-7250(v1.0,v2.0),MS-7260,MS-7279,MS-7280
	

OS : Windows 98/Me/2000/Xp

	version 1.0.0.1 (03/27/03)
			new release
			smartly load saved or auto_overclock frequency & voltages
			startup folder & unstall PC Alert4
		new mainboard : 
         		MS-6728 (ClockGen :ICS 952611BF,Linear over clock , watch-dog , SouthBridge:INTEL 82801ER,NorthBridge:INTEL 865) 
         		MS-6758 (ClockGen :ICS 952611BF,Linear over clock , watch-dog , SouthBridge:INTEL 82801ER,NorthBridge:INTEL 875) 
 	
	version 1.0.0.2 (04/17/03)	
			add version information
			relocate two wings' position
			fix MS-6758 magazine version bug(memory voltage 2.8v,FSB 200 MHz)
			avoid "ini not found" bug
			fix MS-6728 magazine version bug(memory voltage 2.8v,FSB 200 MHz,Vcore 1.55v,close turbo pin)

	version 1.0.5.2 (05/30/03)	
			add version dialog
			add setting of interval time & sound warning
			add historical diagram of CPU & system & NB temperatures 
		new mainboard : 
         		MS-6585 v5.0 (ClockGen :ICS 952011BF,Linear over clock , watch-dog , SouthBridge: Sis963L,NorthBridge:Sis648FX) 

	version 1.5.3.0 (06/09/03)	
			fix auto mode conflict with OM CD setup
			fix bitmap bug when taskbar at top 
			fix clockgen value (FSB=200 MHz) & remove system fan 
		new mainboard : 
         		MS-6788 (ClockGen :ICS 952619CF,Linear over clock , watch-dog , SouthBridge: Intel 82801EB,NorthBridge:Intel 865) 
         		MS-6590 v2.0(ClockGen :ICS 93738AF,Linear over clock , watch-dog , SouthBridge: Via VT8237,NorthBridge:Via KT600) 
         		MS-6799 (ClockGen :ICS 950909AF,Linear over clock , watch-dog , SouthBridge: Via VT8237,NorthBridge:Via PT800) 

	version 1.5.4.0 (07/16/03)	
			add OC menu for MS-6788
			update MS-6788 Vcore adjustment
			fix user fan control save bug
		new mainboard : 
         		MS-6702 (ClockGen :ICS 950403CF,Linear over clock , watch-dog , SouthBridge: Via VT8237,NorthBridge:Via KT800) 
	
	version 1.5.5.0 (08/08/03)	
			add CoolnQuiet for MS-6702
			fix smbus base address for MS-6799 (0x500,Award bios)
			fix voltage adjustment for MS-6758

	version 1.5.6.0 (29/08/03)	
			support MS-6702 magazine version

	version 1.5.6.1 (08/09/03)	
			support MS-7003 (ClockGen :ICS 951402AG,watch-dog,Linear over clock,SouthBridge:ATI IXP150,NorthBridge:ATI RS300) 

	version 1.5.7.0 (09/09/03)	
			support Cool'N'Quiet for MS-6702
			fix MS-6799 new clockgen ICS 950917
		new mainboard : 
			MS-6728 v2.0 (ClockGen :ICS 952611BF,Linear over clock , watch-dog , SouthBridge: Intel 82801EB,NorthBridge:INTEL 865)  
			MS-7008 (ClockGen :ICS 952911AF,Linear over clock , watch-dog , SouthBridge: Via VT8237,NorthBridge:Via PT800)  

	version 1.5.7.1 (10/03/03)
			Add IGP/AGP bitmap for MS-7003

	version 1.5.8.0 (10/01/03)
			add fan control for MS-6728 v2.0c
		new mainboard : 
 			MS-7021 (ClockGen :ICS 950916BF,Linear over clock , watch-dog , SouthBridge: Via VT8237,NorthBridge:Via KT600)  
 			MS-6580 v5.0 (ClockGen :ICS 952611BF,Linear over clock , watch-dog , SouthBridge: Intel 82801EB,NorthBridge:INTEL 845PE)  
	
	version 1.5.9.0 (10/14/03)
			auto overclock interval 6 sec
			add OC menu for MS-7008
			fix fan control for MS-6702
			remove OC menu for MS-6580 v5.0

	version 1.6.0.0 (11/12/03)
			fix OC menu default function
			update M,N value for FSB above 200 MHz
			increase fan control level if fan rpm=0 for auto mode
                        fix FSB200 issue
			fix Prescott CPU Vcore 
			add version information for Live Update

	version 1.6.1.0 (12/26/03)
			merge MS-7003
		new mainboard : 
			MS-6758 v2.0 (ClockGen :ICS 952611BF,Linear over clock , watch-dog , SouthBridge: Intel 82801EB,NorthBridge:INTEL 875)
	
	version 1.6.2.0 (1/28/04)
			fix Japanese OS bitmap offset (width becomes larger) 
			fix Cool&Quiet clock 
			fix fan control while CPU cool down
			fix Prescott CPU Vcore "auto" unselectable
		new mainboard : 
			MS-6788 v2.0 (ClockGen :ICS 952611BF,Linear over clock , watch-dog , SouthBridge: Intel 82801EB,NorthBridge:INTEL 865)
			MS-7043 (ClockGen :ICS 952911BF,Linear over clock , watch-dog , SouthBridge: Via 8237,NorthBridge:Via PT880)

	version 1.6.4.0 (2/26/04)
			fix reboot due to vcore adjustment for MS-6590 v2.0
		new mainboard : 
			MS-7030 (Linear over clock , NForce3 250Gb(CK8S))

	version 1.6.5.0 (3/16/04)
			fix NB fan speed for MS-6728 
			change system fan pic for MS-7047
			reduce cpu fan control range for MS-6570E & MS-6590 v2.0 & MS-7021
		new mainboard : 
			MS-6570E (Linear over clock , NForce2 MCP)
			MS-7025 (Linear over clock , NForce3 250Gb(CK8S))
			MS-7047 (ClockGen :ICS 952930EF,Linear over clock , watch-dog , SouthBridge: Via 8237,NorthBridge:Via KT880)
			MS-6741 (ClockGen :ICS 950403CF,Linear over clock , watch-dog , SouthBridge: Via 8237,NorthBridge:Via KT880)
			MS-7032 (ClockGen :ICS 950410AF,Linear over clock , watch-dog , SouthBridge: Via 8237,NorthBridge:Via KT880)
			MS-6702E (ClockGen :ICS 950410AF,Linear over clock , watch-dog , SouthBridge: Via 8237,NorthBridge:Via KT880)
			MS-7058 (ClockGen :ICS 954129BF,Linear over clock , watch-dog , SouthBridge: Intel 82801FB,NorthBridge:Intel 915G)
	
	version 1.6.6.0 (5/21/04)	
			no fan warning while abnormal speed detected (CPUFanStop ,NBFanStop)
			fix fan speed control (reach full speed)
			Enable fan control function for MS-7058
		new mainboard : 
			MS-7028 (ClockGen :ICS 954130AF,Linear over clock , watch-dog , SouthBridge: Intel 82801FB,NorthBridge:Intel 915G)
			MS-7052 (ClockGen :ICS 954129BF,Linear over clock , watch-dog , SouthBridge: Intel 82801FB,NorthBridge:Intel 915G)
			MS-7031 (ClockGen :ICS 951402AG,Linear over clock , watch-dog , SouthBridge: ATI IXP300,NorthBridge:ATI RS350) 
			MS-7058 (ClockGen :ICS 954139AF/ICS 954129BF,Linear over clock , watch-dog , SouthBridge: Intel 82801FB,NorthBridge:Intel 915G) 

	version 1.6.7.0 (6/04/04)
	        add "bios smart fan control" detecting function.
	        change CPU_SYS_Fan Picture for MS-6702E
	        change "AGP Voltage" picture to "NB Voltage" for MS-7058,MS-7052
	        add "smart fan detecting" for MS-7058
	        fix Vcore function error for MS-7058,MS-7052
	        fix cpu and sys fan speed and fan control error for MS-6702E
		new mainboard : 
			MS-6714 Ver5.0 (ClockGen :Cypress CY28349,Linear over clock , SouthBridge: Intel 82801DB,NorthBridge:Intel 845GE)
	
	version 1.6.8.0 (6/16/04)
		new mainboard : 
			MS-7053 (ClockGen :ICS 954130BF,Linear over clock , watch-dog , SouthBridge: Intel 82801FB,NorthBridge:Intel 925X) 

	version 1.6.9.0 (6/25/04)
		add +12v for MS-7053
		fix cpu temperature for MS-7021
		fix system temp to sensor 3 for MS-7030
		fix overclocking for MS-7028
		MS-6728 Ver1.0 do not show nor bridge temp
		new mainboard : 
			Support MS-6702 v2.0 (ClockGen :ICS 950410AF,Linear over clock , watch-dog , SouthBridge: Via VT8237,NorthBridge:Via K8T800pro) 
                change NB Temp & SYS Temp for MS-7030
	version 1.7.0.0 (8/03/04)
		fix over clock error for MS-7028 (533 MHz CPU)
		new mainboard : 
			MS-6728 Ver3.0 (ClockGen :ICS 952642AF,Linear over clock , watch-dog , SouthBridge: Intel 82801ER,NorthBridge:Intel 865)
		fix watchdog timer error for MS-7028 (CPU:(default FSB: 200 MHz))
		fix CPU fan speed alarm error.
                change "AGP Voltage" picture to "NB Voltage" for MS-7028
		fix vcore setting value error for MS-7028
		fix FSB value error after second boot for MS-7028
		adjust "AGP Voltage" and "Memory Voltage" value order 
		fix "Memory Voltage" value order, adjust "NB Voltage" upper limit and change "Memory Voltage" picture to "DDR Voltage" for MS-7028
		new mainboard : 
			MS-7033 (ClockGen :ICS 954119DF,Linear over clock , watch-dog , SouthBridge: Intel 82801FB,NorthBridge:Intel 915G)
		support CPU fan control for MS-7033
		enable ATI ISA enable bit after S3/S4
		fix vcore & memory voltage adjustment for MS-7025 (MS6)
	version 1.7.1.0 (9/16/04)
		change V33 register mapping for MS-6728 v2(22->21)
		fix Vcore warnning error for MS-6702
		exchange CPU and NB fan speed mapping register addr for MS-6728 v3.0
		adjust DDR and AGP voltage adjustable range for MS-6728 v3.0
                add vcore voltage adjustment for MS-6728 v3.0
		disable fan control function for MS-6728 v3.0 (HW no reserve)
		use MS8 watchdog timer instead of colock gen watchdog timer for MS-6728 v3.0
		fix DDR voltage error(2.8v -> 2.6v) for MS-6758 v1.0
	version 1.7.2.0 (11/04/04)
		add "eveshamvale" for MS-7030 dmi type2 product name string
		add V33 for MS-6702E
		fix system temp to sensor 3 for MS-7025
		new mainboard : 
			MS-7125 (Linear over clock , NForce4(CK804))
			MS-7100 (Linear over clock , NForce4(CK804))
		fix CoolnQuiet picture error for MS-6741
		fix corecenter cpu & system fan error for MS-7125
		new mainboard : 
			MS-7066 (ClockGen:CY28416 , SouthBridge: Intel 82801FB,NorthBridge:Intel 915G)
			MS-7088 (ClockGen:ICS952642AF , SouthBridge: Intel 82801EB,NorthBridge:Intel 865G)
			MS-7133 (ClockGen:ICS954119DF , SouthBridge: Intel 82801FB,NorthBridge:Intel 915)
			MS-7135 (ClockGen:CK8-04 , nVidia CK8-04)
----------------------------------------------------------------------------------------------------
	Author:	Bryan Lin
	New Version: 1.7.3.0	Build Date: 2004.12.08
	Release on CD-73
		a. set INFO.DAT to be non-read-only to fix value can't be saved issue
		b. fix CK8-04 chipset FSB operator
		c. fix CK8-04 Fan Control register position (modify CPU/NB Fan from 03h/01h to be 01h/03h)
		d. modify CPU/NB Fan upper limit to be 9000rpm (MS-7125 NB Fan is over 7000rpm)
----------------------------------------------------------------------------------------------------
	Author:	Bryan Lin
	New Version: 1.7.4.0	Build Date: 2005.01.10	
	Release on CD-74
		a. remove NB Icons if no NB Temperatrue (modify main and right-wing skin)
		b. fix issue that can't detect Hardware Monitor of ATI board (ATIEnableISA in NTGLM7X.SYS) (MS-7003,MS-7031)
----------------------------------------------------------------------------------------------------
	New Version: 1.7.5.0	Build Date: 2005.02.25	
	Release on CD-75
		a. OverClock again after resuming from suspend mode
----------------------------------------------------------------------------------------------------
	New Version: 1.7.6.0	Build Date: 2005.04.09
	Release on new OMCD (IPOM,VPOM,SPOM)
		a. Fan Control(user mode) again after resuming from suspend mode
		b. Fix MS-6702 overclock again failed issue after resuming from suspend mode
		c. Support AMD Semprom 2600+/2800+ K8 CPU
		d. new mainboard : 
			MS-7166 (ClockGen:RTM862-480 , SouthBridge: Intel 82801FB,NorthBridge:Intel 915P)
			MS-7160 (ClockGen:nVidia C19, nVidia C19+MCP4, Linear over clock)
----------------------------------------------------------------------------------------------------
	New Version: 2.0.0.1	Build Date: 2005.04.21
	Release on new OMCD (IPOM,VPOM,SPOM)
		a. fix MS-7160 system hang issue after suspend
		b. fix MS-7160 CPU FSB are wrong issue
		c. fix MS-7160 System Temperature to read Sensor1 (not Sensor3)
		d. change AP version be 2.0.x.x for new OMCD version
		e. support FSB 267MHz (LGA775) CPU for MS-7160
----------------------------------------------------------------------------------------------------
	New Version: 2.0.0.2	Build Date: 2005.05.03
		a. Fan control(auto mode) again after resuming from suspend
		b. new mainboard : 
			MS-7151 (ClockGen:ICS 951416AG, Linear over clock, SouthBridge:ATI IXP400, NorthBridge:ATI RS480)
			MS-7157 (ClockGen:RTM363-213, Linear over clock, SouthBridge:Intel 82801EB, NorthBridge:Intel 848P)
		c. Modify DetectLM78() to auto-get correct ISA IOPort(2E/2F or 4E/4F)
----------------------------------------------------------------------------------------------------
	New Version: 2.0.0.3	Build Date: 2005.05.12
		a. new mainboard : 
			MS-7185 (ClockGen:CK8-04 , nVidia CK8-04) 
			MS-7143 v2X(ClockGen:RTM862-480 , SouthBridge: Intel 82801FB,NorthBridge:Intel 915P) 
----------------------------------------------------------------------------------------------------
	New Version: 2.0.0.4	Build Date: 2005.05.24
		a. fix MS-7058 Fan Control failed issue
		b. remove MS-6728 v2 NB Fan Control Item for FAE request
		c. fix MS-7166 Vcore failed issue
		d. fix auto-get correct ISA IOPort(2E/2F or 4E/4F) failed issue
		e. new mainboard : 
			MS-7176 (ClockGen:ICS 954519BGLF , SouthBridge: Intel 82801GB,NorthBridge:Intel 945P)
		f. patch MS-7166 sys/nb fan location
----------------------------------------------------------------------------------------------------
	New Version: 2.0.0.5	Build Date: 2005.06.21
		a. fix MS-7151 Vcore warning color
		b. enable MS-7160 watch-dog (C19 NB)
		c. correct the show of CK8-04 MB PCI-E clock
----------------------------------------------------------------------------------------------------
	New Version: 2.0.0.6	Build Date: 2005.07.28
		a. completely support MS-7158  (ClockGen:ICS 954519BGLF , watch-dog(MS8), SouthBridge: Intel 82801GB,NorthBridge:Intel 955X)
		b. new mainboard:
			MS-7175 (ClockGen:ICS 954119DF , watch-dog , SouthBridge: Intel 82801FB, NorthBridge: Intel 915)
----------------------------------------------------------------------------------------------------
	New Version: 2.0.0.7	Build Date: 2005.08.25
		a. update Glm7x.dll/NTGlm7x.sys(v0.5.8.22) and RushTop.dll/RushTop.sys(v0.5.8.25) for MS-7194
		b. new mainboard:
			MS-7194 (ClockGen:ICS 951422AGLF, watch-dog, SouthBridge: ATI RD480, NorthBridge: ULi M1573)
		c. update Glm7x.dll/NTGlm7x.sys(v0.5.8.25) for MS-7194
	 	   so, Redefine MS-7194 be SpecialMB=8 for CPU Fan(0x3F)
----------------------------------------------------------------------------------------------------
	New Version: 2.0.0.8	Build Date: 2005.10.25
		a. add MS-7194 cpu/sys fan control
		b. new mainboard : 
			MS-7203 v0B (ClockGen:nVidia C19, nVidia C19+MCP51, watch-dog(C19 NB), Linear over clock)
			MS-7028 v2.0 (ClockGen:ICS 954129BF, Linear over clock , watch-dog(ICS), SouthBridge: Intel 82801FB,NorthBridge:Intel 915P)
			MS-7176 v2.0 (ClockGen:ICS 954519BGLF, Linear over clock , watch-dog(MS7), SouthBridge: Intel 82801GB,NorthBridge:Intel 945PL)
		c. update Glm7x(v0.5.10.12) and RushTop(v0.5.10.11)
		d. add MS-7176 v1.0 watch-dog(MS7)
		e. fix MS-7194 FirstClk parameter failed issue(becuase one K8 4600 cpu can over colck exceed 267MHz)
		f. update RushTop.sys(v0.5.10.24) and nTune 3.00.14.05 API for
		   	MS-7220 (ClockGen:nVidia CK804, nVidia C51D+CK804, percent over clock)
----------------------------------------------------------------------------------------------------
	New Version: 2.0.0.9	Build Date: 2005.11.11
		a. change MS-7176 v2.0 linear over clock to be PERCENT (avoid over certain FSB then reboot, cause no display issue)
		b. support 64bit XP (update RushTop v0.5.11.2)
		c. correct MS-7220 CPU Voltage adjustment
		d. add ICS954519BGLF M/N Enable bit(Byte1) for MS-7176 v2 (its default fsb(200) disable Byte1)
----------------------------------------------------------------------------------------------------
	New Version: 2.0.1.0	Build Date: 2005.11.21
		a. new mainboard : 
			MS-7236 (ClockGen:ICS 954519BGLF, Linear over clock , watch-dog(MS7), SouthBridge: Intel 82801GB,NorthBridge:Intel 945PL)
		b. fix MS-7160 (C19,C51 etc.) ratio error when nTune running
		c. fix MS-7203 v0B NB Fan warning failed issue
----------------------------------------------------------------------------------------------------
	New Version: 2.0.1.1	Build Date: 2005.01.16
		a. new mainboard : 
			MS-7125 v3.0 (Chipset: NForce4(CK804), ClockGen: CK804, Percent over clock)
			MS-7246 (ClockGen:ICS 954519BGLF, Linear over clock , watch-dog(MS7), SouthBridge: Intel 82801GB,NorthBridge:Intel 945PL)
			MS-7203 v1.0 (ClockGen:nVidia C19-C1, nVidia C19-C1+MCP51, watch-dog(C19-C1 NB), Linear over clock)
		b. support MS-7100 Performance BIOS v5.09
			- add CPU Voltage to 23.3% and Memory Voltage to 2.90v,3.00v,3.10v
		c. MS-7176 v1.0 system fan show N/A to path HWMonitor disordered issue
----------------------------------------------------------------------------------------------------
	New Version: 2.0.1.2	Build Date: 2005.01.26
		a. new mainboard :
			MS-7125 v3.0A (Chipset: NForce4(CK804), ClockGen: CK804 API, Percent over clock)
----------------------------------------------------------------------------------------------------
	New Version: 2.0.1.3	Build Date: 2005.03.23
		a. new mainboard :
			MS-7260 (Chipset: nVidia MCP55, ClockGen: MCP55 API, Percent over clock)
			MS-7250 (Chipset: nVidia MCP55, ClockGen: MCP55 API, Percent over clock, Percent pci-e over clock)
		b. fix MS-7125 v3.0A CPU Fan Control failed issue and add CPU Voltage item 23.3%
		c. fix fix K8 CPU of nVidia MB Cool'n'Quiet failed issue by detect "IsK8CPU" first in OnInitDialog()
		d. increase MS-6702E(v930 bios) cpu temperature for FAE request
		e. fix CK8S MB default button of FSB will show wrong FSB issue
		f. replace MS-7250 PCI-E with NB voltage, modify DDR Voltage to read/write MS6 CR02
		g. new mainboard :
			MS-7226 (Chipset: nVidia C51D(NB)+MCP55(SB), ClockGen: NV API, Percent over clock)
		h. fix driver via SMBus can't read nVidia CPU Temp. issue
----------------------------------------------------------------------------------------------------
	New Version: 2.0.1.4	Build Date: 2005.04.18
		a. fix MS-7250 v1.0 CPU Voltage can't write issue
		b. change MS-7226 cpu/sys fan icon to be cpu/nb by PM request
----------------------------------------------------------------------------------------------------
	New Version: 2.0.1.5	Build Date: 2005.05.12
		a. new mainboard :
			MS-7250 v2.0 (Chipset: nVidia MCP55, ClockGen: MCP55 API, Percent over clock)
		b. change MS-7250 v1.0 cpu temp to read SMBus(bios suggestion, original is read ISA Sensor2)
		c. fix MS-7236 default button of FSB will show wrong FSB issue
		d. modify MS-7125 v3.A DMI Check from "3.0A" to "3.A" for BIOS v710
----------------------------------------------------------------------------------------------------
	New Version: 2.0.1.6	Build Date: 2005.05.25
		a. new mainboard :
			MS-7280 v0A (Chipset: ATI RD580+SB600, ClockGen: ICS 951462AGLF, Linear over clock)
		b. change MS-7226 v1.0 MS6 SMBus Base from 0x2D00 to 0x2E00 (by HW changed)
		c. fix saved fsb will overclock wrong when different fsb CPU(133,200) exchange overclocking(MS-7236)
		d. new mainboard :
			MS-7279 v1.0 (Chipset: Intel P965E+ICH7, ClockGen: ICS 9LPRS510CGLF, Linear over clock, watch-dog(MS7))
		e. change MS-7250 (v1.0,v2.0) CPU Temp. reading from 0x00h to 0x01h by BIOS suggestion
		f. support MS-7280 v1.0
			- modify CPUFANIN1(0x3Fh) -> CPUFANIN0(0x29h) by pcb changed
			- modify CPU Temp. reading from FinTek 75383 by pcb changed
			- modify CPU voltage operation in "apply" function
		g. new mainboard :
			MS-7235 v1.0 (Chipset: Intel P965+ICH8, ClockGen: ICS 9LPRS510CGLF)
----------------------------------------------------------------------------------------------------