[Version]
LayoutFile=LAYOUT.INF, layout1.inf, layout2.inf
signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider=%Philips%
; _OEM_  Enter name of .cat file from WHQL, containing the digital signature.
; _OEM_  The catalog file has to be in the same location as the INF file.
CatalogFile=cap7134.cat
DriverVer=10/29/2003, 2.3.1.2.02

[Manufacturer]
%Philips%=Philips

[DestinationDirs]
Cap7134.CopyDrivers = 10,system32\drivers
KSUpdate.Dll = 11

[SourceDisksNames]
1=%DiskName%,,

[SourceDisksFiles]
cap7134.sys=1
34api.dll=1
34pciurd.dll=1
34i2curd.dll=1
34dd.dll=1
34ds.dll=1
34dialog.dll=1
34dlg2.dll=1
34TvCtrl.dll=1
34com.dll=1
Prop7134.dll=1
cap7134.hlp=1

[Philips]

%Cap7134.DeviceFM1216ME%=Cap7134.FM1216ME,PCI\VEN_1131&DEV_7134&SUBSYS_235c1131
%Cap7134.DeviceFQ1216ME%=Cap7134.FQ1216ME,PCI\VEN_1131&DEV_7134&SUBSYS_235d1131 
%Cap7134.TNF8532BF% = Cap7134.TNF8532BF,PCI\VEN_1131&DEV_7134&SUBSYS_23341131
%Cap7134.TNF8532DF% = Cap7134.TNF8532DF,PCI\VEN_1131&DEV_7134&SUBSYS_23351131
%Cap7134.TCL2002MI3% = Cap7134.TCLMI3,PCI\VEN_1131&DEV_7134&SUBSYS_23041131
%Cap7134.TCL2002MB3% = Cap7134.TCLMB3,PCI\VEN_1131&DEV_7134&SUBSYS_23051131
%Cap7134.TCL2002MI1F% = Cap7134.TCLMI1F,PCI\VEN_1131&DEV_7134&SUBSYS_230b1131
%Cap7134.TCL2002N6A% = Cap7134.TCLN6A,PCI\VEN_1131&DEV_7134&SUBSYS_23111131
%Cap7134.TCL2002NJ5% = Cap7134.TCLNJ5,PCI\VEN_1131&DEV_7134&SUBSYS_23031131
%Cap7134.TCL9809N1F% = Cap7134.TCLN1F,PCI\VEN_1131&DEV_7134&SUBSYS_230F1131
%Cap7134.TCL2002MB33F% = Cap7134.TCLM33F,PCI\VEN_1131&DEV_7134&SUBSYS_230E1131

%Cap7130.DeviceFM1216ME%=Cap7134.FM1216ME,PCI\VEN_1131&DEV_7130&SUBSYS_235c1131
%Cap7130.DeviceFQ1216ME%=Cap7134.FQ1216ME,PCI\VEN_1131&DEV_7130&SUBSYS_235d1131 
%Cap7130.TNF8532BF% = Cap7134.TNF8532BF,PCI\VEN_1131&DEV_7130&SUBSYS_23341131
%Cap7130.TNF8532DF% = Cap7134.TNF8532DF,PCI\VEN_1131&DEV_7130&SUBSYS_23351131
%Cap7130.TCL2002MI3% = Cap7134.TCLMI3,PCI\VEN_1131&DEV_7130&SUBSYS_23041131
%Cap7130.TCL2002MB3% = Cap7134.TCLMB3,PCI\VEN_1131&DEV_7130&SUBSYS_23051131
%Cap7130.TCL2002MI1F% = Cap7134.TCLMI1F,PCI\VEN_1131&DEV_7130&SUBSYS_230b1131
%Cap7130.TCL2002N6A% = Cap7134.TCLN6A,PCI\VEN_1131&DEV_7130&SUBSYS_23111131
%Cap7130.TCL2002NJ5% = Cap7134.TCLNJ5,PCI\VEN_1131&DEV_7130&SUBSYS_23031131
%Cap7130.TCL9809N1F% = Cap7134.TCLN1F,PCI\VEN_1131&DEV_7130&SUBSYS_230F1131
%Cap7130.TCL2002MB33F% = Cap7134.TCLM33F,PCI\VEN_1131&DEV_7130&SUBSYS_230E1131











[Cap7134.Device]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration
AddReg=       TCL2002MI3.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg, Prop7134.AddReg, 34COM.AddReg
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll
KnownFiles=   Cap7134.KnownFiles

[Cap7134.Device.NT]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration.NT
AddReg=       TCL2002MI3.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg
RegisterDlls= Prop7134.Register, 34COM.Register
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll

[Cap7134.FM1216ME]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration
AddReg=       FM1216.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg, Prop7134.AddReg, 34COM.AddReg
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll
KnownFiles=   Cap7134.KnownFiles

[Cap7134.FM1216ME.NT]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration.NT
AddReg=       FM1216.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg
RegisterDlls= Prop7134.Register, 34COM.Register
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll

[Cap7134.FQ1216ME]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration
AddReg=       FQ1216ME.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg, Prop7134.AddReg, 34COM.AddReg
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll
KnownFiles=   Cap7134.KnownFiles

[Cap7134.FQ1216ME.NT]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration.NT
AddReg=       FQ1216ME.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg
RegisterDlls= Prop7134.Register, 34COM.Register
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll

[Cap7134.TNF8532BF]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration
AddReg=       TNF8532BF.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg, Prop7134.AddReg, 34COM.AddReg
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll
KnownFiles=   Cap7134.KnownFiles

[Cap7134.TNF8532BF.NT]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration.NT
AddReg=       TNF8532BF.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg
RegisterDlls= Prop7134.Register, 34COM.Register
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll

[Cap7134.TNF8532DF]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration
AddReg=       TNF8532DF.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg, Prop7134.AddReg, 34COM.AddReg
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll
KnownFiles=   Cap7134.KnownFiles

[Cap7134.TNF8532DF.NT]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration.NT
AddReg=       TNF8532DF.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg
RegisterDlls= Prop7134.Register, 34COM.Register
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll

[Cap7134.TCLMI3]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration
AddReg=       TCL2002MI3.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg, Prop7134.AddReg, 34COM.AddReg
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll
KnownFiles=   Cap7134.KnownFiles

[Cap7134.TCLMI3.NT]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration.NT
AddReg=       TCL2002MI3.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg
RegisterDlls= Prop7134.Register, 34COM.Register
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll

[Cap7134.TCLMB3]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration
AddReg=       TCL2002MB3.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg, Prop7134.AddReg, 34COM.AddReg
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll
KnownFiles=   Cap7134.KnownFiles

[Cap7134.TCLMB3.NT]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration.NT
AddReg=       TCL2002MB3.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg
RegisterDlls= Prop7134.Register, 34COM.Register
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll

[Cap7134.TCLMI1F]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration
AddReg=       TCL2002MI1F.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg, Prop7134.AddReg, 34COM.AddReg
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll
KnownFiles=   Cap7134.KnownFiles

[Cap7134.TCLMI1F.NT]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration.NT
AddReg=       TCL2002MI1F.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg
RegisterDlls= Prop7134.Register, 34COM.Register
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll

[Cap7134.TCLN6A]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration
AddReg=       TCL2002N6A.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg, Prop7134.AddReg, 34COM.AddReg
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll
KnownFiles=   Cap7134.KnownFiles

[Cap7134.TCLN6A.NT]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration.NT
AddReg=       TCL2002N6A.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg
RegisterDlls= Prop7134.Register, 34COM.Register
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll

[Cap7134.TCLNJ5]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration
AddReg=       TCL2002NJ5.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg, Prop7134.AddReg, 34COM.AddReg
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll
KnownFiles=   Cap7134.KnownFiles

[Cap7134.TCLNJ5.NT]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration.NT
AddReg=       TCL2002NJ5.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg
RegisterDlls= Prop7134.Register, 34COM.Register
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll

[Cap7134.TCLN1F]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration
AddReg=       TCL9809N1F.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg, Prop7134.AddReg, 34COM.AddReg
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll
KnownFiles=   Cap7134.KnownFiles

[Cap7134.TCLN1F.NT]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration.NT
AddReg=       TCL9809N1F.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg
RegisterDlls= Prop7134.Register, 34COM.Register
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll

[Cap7134.TCLM33F]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration
AddReg=       TCL2002MB33F.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg, Prop7134.AddReg, 34COM.AddReg
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll
KnownFiles=   Cap7134.KnownFiles

[Cap7134.TCLM33F.NT]
Include=      ks.inf, kscaptur.inf, ksfilter.inf
Needs=        KS.Registration, KSCAPTUR.Registration.NT
AddReg=       TCL2002MB33F.AddReg, Cap713x.AddRegProteus, Cap7134.AddReg, Cap713x.AddReg
RegisterDlls= Prop7134.Register, 34COM.Register
CopyFiles=    Cap7134.CopyDrivers, KSUpdate.Dll










[Cap713x.AddRegProteus]
HKR, "Decoder", "Tuner Channel",0x00010001,1
HKR, "Decoder", "CVBS Channel",0x00010001,3
HKR, "Decoder", "CVBS Channel2",0x00010001,3
HKR, "Decoder", "SVHS Channel",0x00010001,6
HKR, "Decoder", "SVHS Channel2",0x00010001,7
; _OEM_  Insert the appropriate preferred video standard here.
; _OEM_  If no video standard can be detected (e.g. if no
; _OEM_  video source is connected), this standard is assumed:
; _OEM_     KS_AnalogVideo_PAL_B    = 0x00000010
; _OEM_     KS_AnalogVideo_NTSC_M   = 0x00000001
; _OEM_     KS_AnalogVideo_NTSC_M_J = 0x00000002
; _OEM_     see Windows DDK for other video standards
HKR, "Decoder", "Preferred Video Standard",0x00010001,0x00000010    ; KS_AnalogVideo_PAL_B
; _OEM_  Insert the default VBI sampling frequency and line length here.
HKR, "Decoder", "VBI Sampling Frequency",0x00010001,27000000
HKR, "Decoder", "VBI Pitch",0x00010001,1440

[FM1216.AddReg] 
; _OEM_  Delete this line if there is no tuner or replace
; _OEM_  "PhTVTune" with the appropriate tuner driver name.
HKR, "ENUM\Device1",pnpid,,"PhTVFM"

[FQ1216ME.AddReg] 
; _OEM_  Delete this line if there is no tuner or replace
; _OEM_  "PhTVTune" with the appropriate tuner driver name.
HKR, "ENUM\Device1",pnpid,,"PhTVFQ"

[TNF8532BF.AddReg] 
; _OEM_  Delete this line if there is no tuner or replace
; _OEM_  "PhTVTune" with the appropriate tuner driver name.
HKR, "ENUM\Device1",pnpid,,"PhTVBF"

[TNF8532DF.AddReg] 
; _OEM_  Delete this line if there is no tuner or replace
; _OEM_  "PhTVTune" with the appropriate tuner driver name.
HKR, "ENUM\Device1",pnpid,,"PhTVDF"

[TCL2002MI3.AddReg] 
; _OEM_  Delete this line if there is no tuner or replace
; _OEM_  "PhTVTune" with the appropriate tuner driver name.
HKR, "ENUM\Device1",pnpid,,"PhTMI3"

[TCL2002MB3.AddReg] 
; _OEM_  Delete this line if there is no tuner or replace
; _OEM_  "PhTVTune" with the appropriate tuner driver name.
HKR, "ENUM\Device1",pnpid,,"PhTMB3"

[TCL2002MI1F.AddReg] 
; _OEM_  Delete this line if there is no tuner or replace
; _OEM_  "PhTVTune" with the appropriate tuner driver name.
HKR, "ENUM\Device1",pnpid,,"PhTMI1F"

[TCL2002N6A.AddReg] 
; _OEM_  Delete this line if there is no tuner or replace
; _OEM_  "PhTVTune" with the appropriate tuner driver name.
HKR, "ENUM\Device1",pnpid,,"PhTN6A"

[TCL2002NJ5.AddReg] 
; _OEM_  Delete this line if there is no tuner or replace
; _OEM_  "PhTVTune" with the appropriate tuner driver name.
HKR, "ENUM\Device1",pnpid,,"PhTNJ5"

[TCL9809N1F.AddReg] 
; _OEM_  Delete this line if there is no tuner or replace
; _OEM_  "PhTVTune" with the appropriate tuner driver name.
HKR, "ENUM\Device1",pnpid,,"PhTN1F"

[TCL2002MB33F.AddReg] 
; _OEM_  Delete this line if there is no tuner or replace
; _OEM_  "PhTVTune" with the appropriate tuner driver name.
HKR, "ENUM\Device1",pnpid,,"PhTM33F"









;Common registry entries for SAA7134 and SAA7130
[Cap713x.AddReg]
; 34 Proteus Board Settings
; maps user setting to hardware input (1=SIF, 2=Analog1, 3=Analog2)  
HKR, "BoardSetting", "Tuner",0x00010001,1
HKR, "BoardSetting", "Composite1",0x00010001,2
HKR, "BoardSetting", "SVideo1",0x00010001,2
HKR, "BoardSetting", "Composite2",0x00010001,3
HKR, "BoardSetting", "SVideo2",0x00010001,3
HKR, "BoardSetting", "FM",0x00010001,3

HKR, "", "WorkaroundforStandardChange",0x00010001,0

HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,Cap7134.sys
HKR,,PageOutWhenUnopened,3,0
HKR,,DontSuspendIfStreamsAreRunning,3,00
HKR, "Parameters", "VideoTunerEnabled",0x00010001,1
HKR, "Parameters", "SVideoEnabled",0x00010001,1
HKR, "Parameters", "CompositeEnabled",0x00010001,1

; _OEM_  Delete this line if there is no tuner or replace
; _OEM_  "PhTVTune" with the appropriate tuner driver name.
;HKR, "ENUM\Device1",pnpid,,"PhTVTune"

;>>> decoder defaults for tuner input
HKR, "Decoder\SRC0", "Brightness",0x00010001,0x80
HKR, "Decoder\SRC0", "Contrast",0x00010001,0x44
HKR, "Decoder\SRC0", "Saturation",0x00010001,0x40
HKR, "Decoder\SRC0", "HUE",0x00010001,0x00
HKR, "Decoder\SRC0", "Sharpness",0x00010001,0x00
HKR, "Decoder\SRC0", "Source Type",0x00010001,0x02
HKR, "Decoder\SRC0", "Y-Filter",0x00010001,0x01
HKR, "Decoder\SRC0", "C-Filter",0x00010001,0x01
HKR, "Decoder\SRC0", "C-Bypass",0x00010001,0x00
;>>>  decoder defaults for composite 1 source
HKR, "Decoder\SRC1", "Brightness",0x00010001,0x80
HKR, "Decoder\SRC1", "Contrast",0x00010001,0x44
HKR, "Decoder\SRC1", "Saturation",0x00010001,0x40
HKR, "Decoder\SRC1", "HUE",0x00010001,0x00
HKR, "Decoder\SRC1", "Sharpness",0x00010001,0x00
HKR, "Decoder\SRC1", "Source Type",0x00010001,0x02
HKR, "Decoder\SRC1", "Y-Filter",0x00010001,0x01
HKR, "Decoder\SRC1", "C-Filter",0x00010001,0x01
HKR, "Decoder\SRC1", "C-Bypass",0x00010001,0x00
;>>>  decoder defaults for composite 2 source
HKR, "Decoder\SRC2", "Brightness",0x00010001,0x80
HKR, "Decoder\SRC2", "Contrast",0x00010001,0x44
HKR, "Decoder\SRC2", "Saturation",0x00010001,0x40
HKR, "Decoder\SRC2", "HUE",0x00010001,0x00
HKR, "Decoder\SRC2", "Sharpness",0x00010001,0x00
HKR, "Decoder\SRC2", "Source Type",0x00010001,0x02
HKR, "Decoder\SRC2", "Y-Filter",0x00010001,0x01
HKR, "Decoder\SRC2", "C-Filter",0x00010001,0x01
HKR, "Decoder\SRC2", "C-Bypass",0x00010001,0x00
;>>>  decoder defaults for SVHS 1 source
HKR, "Decoder\SRC3", "Brightness",0x00010001,0x80
HKR, "Decoder\SRC3", "Contrast",0x00010001,0x44
HKR, "Decoder\SRC3", "Saturation",0x00010001,0x40
HKR, "Decoder\SRC3", "HUE",0x00010001,0x00
HKR, "Decoder\SRC3", "Sharpness",0x00010001,0x00
HKR, "Decoder\SRC3", "Source Type",0x00010001,0x02
HKR, "Decoder\SRC3", "Y-Filter",0x00010001,0x00
HKR, "Decoder\SRC3", "C-Filter",0x00010001,0x00
HKR, "Decoder\SRC3", "C-Bypass",0x00010001,0x01
;>>>  decoder defaults for SVHS 2 source
HKR, "Decoder\SRC4", "Brightness",0x00010001,0x80
HKR, "Decoder\SRC4", "Contrast",0x00010001,0x44
HKR, "Decoder\SRC4", "Saturation",0x00010001,0x40
HKR, "Decoder\SRC4", "HUE",0x00010001,0x00
HKR, "Decoder\SRC4", "Sharpness",0x00010001,0x00
HKR, "Decoder\SRC4", "Source Type",0x00010001,0x02
HKR, "Decoder\SRC4", "Y-Filter",0x00010001,0x00
HKR, "Decoder\SRC4", "C-Filter",0x00010001,0x00
HKR, "Decoder\SRC4", "C-Bypass",0x00010001,0x01

;Registry entries irrelevant for SAA7130
[Cap7134.AddReg]
HKR,,Driver,,Cap7134.sys

; possible 'software' audio enable/disable switch (0=disable,1=enable) 
HKR, "Parameters", "AudioEnabled",0x00010001,1          ; enable audio
HKR, "Parameters", "AudioTunerEnabled",0x00010001,1     ; enable tuner audio

;>>> audio settings for tuner input

; 'CountryCode' reflects the used Country
; and is used as a table entry to 'DefaultStandard' and 'StandardTable'
; in order to perform a country dependant audio standard search
; _OEM_  Enter the appropriate country code here
HKR, "", "CountryCode",,"49"   ; Germany

; 'XTAL' reflects the used hardware crystal (0=32.11MHz,1=24.567MHz)
HKR, "Audio", "XTAL",0x00010001,0x01

; 'DetectMode' reflects the used audio detection mode (1=automatic mode,0=manual mode)
HKR, "Audio", "DetectMode",0x00010001,0x01          ; automatic mode

; 'DefaultStandard'
; in automatic mode: 'DefaultStandard' is used as a fallback if nothing is detected
; in manual mode:    'DefaultStandard' is used as standard to be set
;   2  = B/G   Mono           
;   3  = D/K   Mono           
;   4  = M     Mono           
;   5  = B/G   A2
;   6  = B/G   Nicam
;   7  = D/K   A2 Type 1
;   8  = D/K   A2 Type 2
;   9  = D/K   A2 Type 3
;   10 = D/K   Nicam
;   11 = L/L'  Nicam
;   12 = L/L'  AM
;   13 = I     Nicam
;   14 = I     Mono
;   15 = M     Korea
;   16 = M     BTSC
HKR, "Audio\DefaultStandard", "01",0x00010001,16   ; USA:           M    BTSC
HKR, "Audio\DefaultStandard", "31",0x00010001,5    ; Netherlands:   B/G  A2
HKR, "Audio\DefaultStandard", "32",0x00010001,6    ; Belgium:       B/G  Nicam
HKR, "Audio\DefaultStandard", "33",0x00010001,11   ; France:        L/L' Nicam
HKR, "Audio\DefaultStandard", "34",0x00010001,5    ; Spain:         B/G  A2
HKR, "Audio\DefaultStandard", "39",0x00010001,5    ; Italy:         B/G  A2
HKR, "Audio\DefaultStandard", "41",0x00010001,5    ; Switzerland:   B/G  A2
HKR, "Audio\DefaultStandard", "44",0x00010001,13   ; Great Britain: I    Nicam
HKR, "Audio\DefaultStandard", "45",0x00010001,6    ; Denmark        B/G  Nicam
HKR, "Audio\DefaultStandard", "46",0x00010001,6    ; Sweden:        B/G  Nicam
HKR, "Audio\DefaultStandard", "47",0x00010001,6    ; Norway:        B/G  Nicam
HKR, "Audio\DefaultStandard", "49",0x00010001,5    ; Germany:       B/G  A2
HKR, "Audio\DefaultStandard", "81",0x00010001,16   ; Japan:         M    BTSC
HKR, "Audio\DefaultStandard", "86",0x00010001,7    ; China:         D/K  A2 Type 1
HKR, "Audio\DefaultStandard","351",0x00010001,5    ; Azores:        B/G  A2
HKR, "Audio\DefaultStandard","358",0x00010001,6    ; Finland:       B/G  Nicam
HKR, "Audio\DefaultStandard","420",0x00010001,10   ; Czech Republic:D/K  Nicam

; 'StandardTable'
; in automatic mode: StandardTable is used to set the standard groups to be searched
; bit array:
;   bit1 = B/G
;   bit2 = D/K
;   bit3 = L/L'
;   bit4 = I
;   bit5 = M
HKR, "Audio\StandardTable", "01",0x00010001,0x10   ; USA:           M
HKR, "Audio\StandardTable", "31",0x00010001,0x01   ; Netherlands:   B/G
HKR, "Audio\StandardTable", "32",0x00010001,0x01   ; Belgium:       B/G
HKR, "Audio\StandardTable", "33",0x00010001,0x04   ; France:        L/L'
HKR, "Audio\StandardTable", "34",0x00010001,0x01   ; Spain:         B/G
HKR, "Audio\StandardTable", "39",0x00010001,0x01   ; Italy:         B/G
HKR, "Audio\StandardTable", "41",0x00010001,0x01   ; Switzerland:   B/G
HKR, "Audio\StandardTable", "44",0x00010001,0x08   ; Great Britain: I
HKR, "Audio\StandardTable", "45",0x00010001,0x01   ; Denmark        B/G
HKR, "Audio\StandardTable", "46",0x00010001,0x01   ; Sweden:        B/G
HKR, "Audio\StandardTable", "47",0x00010001,0x01   ; Norway:        B/G
HKR, "Audio\StandardTable", "49",0x00010001,0x01   ; Germany:       B/G
HKR, "Audio\StandardTable", "81",0x00010001,0x10   ; Japan:         M
HKR, "Audio\StandardTable", "86",0x00010001,0x02   ; China:         D/K
HKR, "Audio\StandardTable","351",0x00010001,0x01   ; Azores:        B/G
HKR, "Audio\StandardTable","358",0x00010001,0x01   ; Finland:       B/G
HKR, "Audio\StandardTable","420",0x00010001,0x02   ; Czech Republic:D/K

[Cap7134.CopyDrivers]
Cap7134.sys

[Cap7134.KnownFiles]
Cap7134.sys=safe

[Cap7134.Device.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},"GLOBAL",VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TVAudio

[Cap7134.Device.NT.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%refGlobal%,VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},%refGlobal%,VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,TVAudio

[Cap7134.FM1216ME.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},"GLOBAL",VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TVAudio

[Cap7134.FM1216ME.NT.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%refGlobal%,VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},%refGlobal%,VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,TVAudio

;FQ1216ME
[Cap7134.FQ1216ME.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},"GLOBAL",VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TVAudio

[Cap7134.FQ1216ME.NT.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%refGlobal%,VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},%refGlobal%,VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,TVAudio

[Cap7134.TNF8532BF.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},"GLOBAL",VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TVAudio

[Cap7134.TNF8532BF.NT.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%refGlobal%,VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},%refGlobal%,VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,TVAudio

[Cap7134.TNF8532DF.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},"GLOBAL",VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TVAudio

[Cap7134.TNF8532DF.NT.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%refGlobal%,VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},%refGlobal%,VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,TVAudio

[Cap7134.TCLMI3.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},"GLOBAL",VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TVAudio

[Cap7134.TCLMB3.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},"GLOBAL",VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TVAudio

[Cap7134.TCLMI3.NT.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%refGlobal%,VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},%refGlobal%,VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,TVAudio

[Cap7134.TCLMB3.NT.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%refGlobal%,VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},%refGlobal%,VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,TVAudio

[Cap7134.TCLMI1F.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},"GLOBAL",VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TVAudio

[Cap7134.TCLMI1F.NT.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%refGlobal%,VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},%refGlobal%,VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,TVAudio

;TCLN6A
[Cap7134.TCLN6A.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},"GLOBAL",VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TVAudio

[Cap7134.TCLN6A.NT.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%refGlobal%,VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},%refGlobal%,VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,TVAudio

[Cap7134.TCLNJ5.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},"GLOBAL",VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TVAudio

[Cap7134.TCLNJ5.NT.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%refGlobal%,VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},%refGlobal%,VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,TVAudio

[Cap7134.TCLN1F.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},"GLOBAL",VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TVAudio

[Cap7134.TCLN1F.NT.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%refGlobal%,VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},%refGlobal%,VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,TVAudio

[Cap7134.TCLM33F.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},"GLOBAL",VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},"GLOBAL",VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TVAudio

[Cap7134.TCLM33F.NT.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%refGlobal%,VideoCapture
AddInterface={6994AD05-93EF-11D0-A3CC-00A0C9223196},%refGlobal%,VideoCapture
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,VideoCrossbar
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%refGlobal%,TVAudio












[KSUpdate.Dll]
34api.dll
34pciurd.dll
34i2curd.dll
34dd.dll
34ds.dll
34dialog.dll
34dlg2.dll
34TvCtrl.dll
34com.dll
Prop7134.dll      ; audio property dialog
cap7134.hlp

[VideoCapture]
AddReg=VideoCapture.AddReg

[VideoCrossbar]
AddReg=VideoXBar.AddReg

[TVAudio]
AddReg=TVAudio.AddReg

[VideoCapture.AddReg]
HKR,,CLSID,,{17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%Cap7134.Capture%
; 
; The following entries are used by the PhilipsTV sample application:
; _OEM_  Enter the country name
HKLM,"Software\Philips Semiconductors\SAA7134","Country",,"germany"
; _OEM_  Enter the tuner type
HKLM,"Software\Philips Semiconductors\SAA7134","Tuner",,"FM1216ME"
HKLM,"Software\Philips Semiconductors\SAA7134","TunerSlaveAdress",0x00010001,0xC0
HKLM,"Software\Philips Semiconductors\SAA7134\PhiViA","UseOverlaySurface",0x00010001,1
HKLM,"Software\Philips Semiconductors\SAA7134\VidCap","UseOverlaySurface",0x00010001,1
HKLM,"Software\Philips Semiconductors\SAA7134\VidCap","In_Height_50Hz",0x00010001,288
HKLM,"Software\Philips Semiconductors\SAA7134\VidCap","In_Height_60Hz",0x00010001,240
HKLM,"Software\Philips Semiconductors\SAA7134\VidCap","In_StartX_50Hz",0x00010001,10
HKLM,"Software\Philips Semiconductors\SAA7134\VidCap","In_StartY_50Hz",0x00010001,24
HKLM,"Software\Philips Semiconductors\SAA7134\VidCap","In_Width_50Hz",0x00010001,702
HKLM,"Software\Philips Semiconductors\SAA7134\VidCap","In_StartX_60Hz",0x00010001,10
HKLM,"Software\Philips Semiconductors\SAA7134\VidCap","In_StartY_60Hz",0x00010001,24
HKLM,"Software\Philips Semiconductors\SAA7134\VidCap","In_Width_60Hz",0x00010001,702
HKLM,SOFTWARE\Intel\Intercast\TVControl,TVControlDLL,,34TVCtrl.dll
HKLM,SOFTWARE\Intel\Intercast\Drivers,biBitCount,,16
HKLM,SOFTWARE\Intel\Intercast\Drivers,biCompression,,BI_RGB
HKLM,SOFTWARE\Intel\Intercast\Drivers,Capture Description,,%Cap7134.Capture%
HKCR,Intercast.Display,DisplayBitMask,,f
; Private Pin Names:
; MEDIATYPE_Audio:
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\{73647561-0000-0010-8000-00AA00389B71},"Name",0x00000000,"Audio"
; GUID_VSB_OUT:
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\{F3954424-34F6-11D1-821D-0000F8300212},"Name",0x00000000,"Transport In"
; MEDIUM_AUDIO_PHILDEC_ANALOGAUDIOIN:
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\{0482DEE1-7817-11cf-8a03-00aa006ecb65},"Name",0x00000000,"Analog Audio In"

[Prop7134.AddReg]
HKLM,Software\Microsoft\Windows\CurrentVersion\RunOnce,"AudioProperties",,"%11%\Regsvr32 /s %11%\Prop7134.dll"

[34COM.AddReg]
HKLM,Software\Microsoft\Windows\CurrentVersion\RunOnce,"COMInterface",,"%11%\Regsvr32 /s %11%\34com.dll"

[Prop7134.Register]
11,,Prop7134.dll,1 ;FLG_REGSVR_DLLREGISTER

[34COM.Register]
11,,34COM.dll,1 ;FLG_REGSVR_DLLREGISTER
   
[VideoXBar.AddReg]
HKR,,CLSID,,{71F96460-78F3-11d0-A18C-00A0C9118956}
HKR,,FriendlyName,,%Cap7134.Crossbar%

[TVAudio.AddReg]
HKR,,CLSID,,{71F96462-78F3-11d0-A18C-00A0C9118956}
HKR,,FriendlyName,,%Cap7134.TVAudio%

[Cap7134.Device.NT.Services]
AddService = Cap7134,0x00000002,Cap7134.ServiceInstall

[Cap7134.FM1216ME.NT.Services]
AddService = Cap7134,0x00000002,Cap7134.ServiceInstall

[Cap7134.FQ1216ME.NT.Services]
AddService = Cap7134,0x00000002,Cap7134.ServiceInstall

[Cap7134.TNF8532BF.NT.Services]
AddService = Cap7134,0x00000002,Cap7134.ServiceInstall

[Cap7134.TNF8532DF.NT.Services]
AddService = Cap7134,0x00000002,Cap7134.ServiceInstall

[Cap7134.TCLMI3.NT.Services]
AddService = Cap7134,0x00000002,Cap7134.ServiceInstall

[Cap7134.TCLMB3.NT.Services]
AddService = Cap7134,0x00000002,Cap7134.ServiceInstall

[Cap7134.TCLMI1F.NT.Services]
AddService = Cap7134,0x00000002,Cap7134.ServiceInstall

;TCLN6A
[Cap7134.TCLN6A.NT.Services]
AddService = Cap7134,0x00000002,Cap7134.ServiceInstall

[Cap7134.TCLNJ5.NT.Services]
AddService = Cap7134,0x00000002,Cap7134.ServiceInstall

[Cap7134.TCLN1F.NT.Services]
AddService = Cap7134,0x00000002,Cap7134.ServiceInstall

[Cap7134.TCLM33F.NT.Services]
AddService = Cap7134,0x00000002,Cap7134.ServiceInstall









[Cap7134.ServiceInstall]
DisplayName   = %Cap7134.Capture%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %12%\Cap7134.sys

;---------------------------------------------------------------
;                S t r i n g s
;---------------------------------------------------------------

[Strings]

;----------------
; Non-Localizable
;----------------

SERVICE_KERNEL_DRIVER=1
SERVICE_ERROR_NORMAL=1
SERVICE_AUTO_START=2
SERVICE_DEMAND_START=3

refGlobal="GLOBAL"
refWave="WAVE"

;----------------
; Localizable
;----------------
Philips			= "10Moons Tech"
DiskName		= "10Moons WDM Video Capture Install disk"
Cap7134.Capture		= "713x_3 TV Card Capture"
Cap7134.Crossbar	= "713x_3 TV Card Crossbar"
Cap7134.TVAudio		= "713x_3 TV Card TV Audio (Proteus)"
Cap7134.DeviceDesc	= "10Moons TV Master3, WDM Video Captures"
Cap7134.DeviceFM1216ME 	= "10Moons TV Master3, WDM Video Captures"
Cap7134.DeviceFQ1216ME 	= "10Moons TV Master3, WDM Video Captures"
Cap7134.TNF8532BF	= "10Moons TV Master3, WDM Video Captures"
Cap7134.TNF8532DF	= "10Moons TV Master3, WDM Video Captures"
Cap7134.TCL2002MI3	= "10Moons TV Master3, WDM Video Captures"
Cap7134.TCL2002MB3	= "10Moons TV Master3, WDM Video Captures"
Cap7134.TCL2002MI1F	= "10Moons TV Master3, WDM Video Captures"
Cap7134.TCL2002N6A	= "10Moons TV Master3, WDM Video Captures"
Cap7134.TCL2002NJ5	= "10Moons TV Master3, WDM Video Captures"
Cap7134.TCL9809N1F      = "10Moons TV Master3, WDM Video Captures"
Cap7134.TCL9809N1F 	= "10Moons TV Master3, WDM Video Captures"
Cap7134.TCL2002MB33F 	= "10Moons TV Master3, WDM Video Captures"

Cap7130.DeviceDesc	= "10Moons TV Master3, WDM Video Captures"
Cap7130.DeviceFM1216ME 	= "10Moons TV Master3, WDM Video Captures"
Cap7130.DeviceFQ1216ME 	= "10Moons TV Master3, WDM Video Captures"
Cap7130.TNF8532BF	= "10Moons TV Master3, WDM Video Captures"
Cap7130.TNF8532DF	= "10Moons TV Master3, WDM Video Captures"
Cap7130.TCL2002MI3	= "10Moons TV Master3, WDM Video Captures"
Cap7130.TCL2002MB3	= "10Moons TV Master3, WDM Video Captures"
Cap7130.TCL2002MI1F	= "10Moons TV Master3, WDM Video Captures"
Cap7130.TCL2002N6A	= "10Moons TV Master3, WDM Video Captures"
Cap7130.TCL2002NJ5	= "10Moons TV Master3, WDM Video Captures"
Cap7130.TCL9809N1F      = "10Moons TV Master3, WDM Video Captures"
Cap7130.TCL9809N1F 	= "10Moons TV Master3, WDM Video Captures"
Cap7130.TCL2002MB33F 	= "10Moons TV Master3, WDM Video Captures"

