Dial!List Help
Index

# Fehlerbehebungen

Overview of frequent errors.

- Preferences not stored
  Your modifications in the preferences are only taken over and saved if you close the preference window. If you made modifications you are requested to save these, to reject or abort and return to the preference window.

- Firewall
  A frequent error why the calling monitor cannot be activated or no connection to the FRITZ!Box cannot be done is, that a Firewall (like LittleSnitch, or the integrated Firewall in Mac OS X) the traffic on port 80 and 1012 blocks. Guarantee that Dial!List has an authorization for this port for in- and outgoing connections.

- Country or City Codes
  If you do not see a picture or contact informatin like a name, although this contact is stored in the Address Book, or not the correct call number is dialed, then you possibly did not deposit the correct country or city code in the preferences.
  Country Code:
  The first text field is for the country prefix. For Germany ist the value 00.
  The second text field is for the country code. For Germany ist the value 49.
  City Code:
  The first text field is for the city prefix. For Germany ist the value 0.
  The second text field is for the city code. For Bamberg ist the value 951.

  In your FRITZ!Box you already input these codes. On this you can orient yourselves. For that open the FRITZ!Box-Webinterface http://fritz.box and navigate to this menu: Settings -> Telephony -> Internettelephony -> Advanced Settings

##