ESNE_SBTE 0xA3 0x0300      "Start SN is bigger than end SN !"                           
ESNE_SNTL 0xA3 0x0301      "Serial number is too long !"                                
                                                                                             
EFRF_CFTV      0x0310 0x10 "Can not find the token value in flash dBase !"                   
EFRF_DFFE      0x0311 0x13 "Decode flash file occurs error !"                                
EFRF_AFOE      0x0312 0x14 "Add flash object occurs error !"                                 
EFRF_MFOE      0x0313 0x15 "To modify flash object occurs error !"                           
EFRF_PFAE      0x0314 0x16 "Put flash object to array occurs error !"                        
EFRF_GFIE      0x0315 0x17 "Get flash object by ID occurs error !"                           
EFRF_FFVE      0x0316 0x18 "The version of flash file has error !"                           
EFRF_CGFF      0x0317 0x19 "Can not get flashDB file !"                                      
EFRF_FPNN      0x0318 0x1A "Flash part number is null !"                                     
EFRF_EDOE      0x0319 0x1B "En/Decode flashDB occurs error !"   
EFRF_VFTO      0x031A 0x1C "The version of FlashDB is too old !"                             
                                                                                             
ECMD_SCOE 0x28 0x0330      "SCSI command occurs error, 1=\"%s\", 2=\"%s\" !"            
ECMD_TDNS      0x0331 0x30 "The device is not support SCSI command !"                        
ECMD_SCOU      0x0332 0x31 "SCSI command occurs unknown error !"   
ECMD_ECOE,     0x0333 0x32 "To execute command occurs error !"                                  
ECMD_AWME      0x0334 0x33 "Allocate writting memory occurs error !"                         
ECMD_SCFS      0x0335 0x34 "SCSI command is forced to stop !"                                
                                                                                             
EDEV_NFMO      0x0360 0x40 "No flash mounted on device !"                                    
EDEV_FCIE      0x0361 0x41 "The flash channel number is not equal !"                         
EDEV_MFTR 0x14 0x0362      "The mounted flash type is not match !"                      
EDEV_FSFC      0x0363 0x42 "The first select and channel is no mount flash !"                
EDEV_FPNM      0x0364 0x43 "The flash mounted position is not match !"                       
EDEV_CAOE      0x0365 0x45 "To convert address occurs error  !"                              
EDEV_BNOR      0x0366 0x46 "The block number is out of range !"                              
EDEV_RPOE      0x0367 0x47 "Read page occurs error !"                                        
EDEV_RSOE      0x0368 0x49 "Read spare occurs error !"                                       
EDEV_WPOE      0x0369 0x4A "Write page occurs error !"                                       
EDEV_WSOE      0x036A 0x4B "Write spare occurs error !"                                      
EDEV_EBOE      0x036B 0x4C "Erase block occurs error !"                                      
EDEV_CTOE      0x036C 0x4D "Check \"%s\" tag occurs error !"                                 
EDEV_NITL      0x036D 0x4E "\"%s\" number is too large !"                                    
EDEV_GDCE      0x036E 0x4F "Getting capacity of device occurs error !"                       
EDEV_GPIE      0x036F 0x50 "Create port info. occurs error !"                                
EDEV_GQRE      0x0370 0x51 "Get quotient and rest occurs error !"                            
EDEV_RFIE      0x0371 0x52 "Read flash ID occurs error !"                                    
EDEV_TFNS 0x12 0x0372      "This flash ID does not support %s !"                        
EDEV_CFII      0x0373 0x53 "Can not find the flash information by index !"                   
EDEV_CMOE      0x0374 0x55 "Copy memory occurs error !"                                      
EDEV_RBOE      0x0375 0x56 "Read block occurs error !"
EDEV_EVBU      0x0376 0x57 "Erase VBs in WBT occurs unknown error !" 
EDEV_RLOE      0x0377 0x58 "Read LUN data occurs error !" 
EDEV_WLOE      0x0378 0x59 "Write LUN data occurs error !"
EDEV_WBOE      0x0379 0x5A "Write block occurs error !"
EDEV_RBBE      0x037A 0x5B "Rebuild bad block occurs error !"
EDEV_RBTM      0x037B 0x5C "To rebuild blocks founded that bad block is too much !
EDEV_CPSE      0x037C 0x5D "Bad page is too much !        
                                                                                
EOTS_MFOE      0x0700 0x70 "Make flash array occurs error !"                                 
EOTS_EFOE 0x68 0x0701      "Block operation occurs error !"                             
EOTS_CBOE      0x0702 0x71 "Create bad block bitmap occurs error !"                          
EOTS_CCOE      0x0703 0x73 "Create CIS table occurs error !"                                 
EOTS_CSOE      0x0704 0x75 "Create system table occurs error !"                          
EOTS_WIOE 0x72 0x0705      "Write ISP code occurs error !"                              
EOTS_CTFC      0x0706 0x76 "Can not find configuration file !"                               
EOTS_WWBE      0x0707 0x77 "Write WBT table occurs error !"                                  
EOTS_CZLE      0x0708 0x78 "Create zone LUT table occurs error !"                            
EOTS_CWUE      0x0709 0x79 "Create WBT table occurs unknown error !"                         
EOTS_CCSE      0x070A 0x7A "To check sum of CIS occurs error !"                              
EOTS_WCOE      0x070B 0x7B "Write CIS table occurs error !"                                  
EOTS_WROE      0x070C 0x7C "Write Root table occurs error !"                                 
EOTS_CSUE      0x070D 0x7D "Create system LUT table occurs unknown error !"                  
EOTS_WLOE      0x070E 0x7E "Write LUT table occurs error !"                                  
EOTS_LNHE      0x070F 0x7F "LUT number has error !"                                          
EOTS_WTOE      0x0710 0x80 "Write TAT table occurs error !"                                  
EOTS_WEOE      0x0711 0x81 "Write EXT table occurs error !"                                  
EOTS_FSUE      0x0712 0x82 "Finished system LUT table occurs unknown error !"                
EOTS_CROE      0x0713 0x83 "To reset of CPU occurs error !"                                  
EOTS_CDOE 0x74 0x0714      "Compare \"%s\" data occurs error !"                         
EOTS_RCOE      0x0715 0x84 "Read CIS table occurs error !"                                   
EOTS_RROE      0x0716 0x85 "Read Root table occurs error !"                                  
EOTS_RBOE      0x0717 0x86 "Reading bad block file occurs error !"                           
EOTS_LBOE      0x0718 0x87 "Loading bad block file occurs error !"                           
EOTS_SECE      0x0719 0x89 "System existence checking occurs error !"                        
EOTS_CCTE 0x88 0x071A      "Copy compare testing occurs error !"                        
EOTS_FONE 0x11 0x071B      "Flash \"%s\" is not match !"                                
EOTS_WSOE      0x071C 0x8A "Write system address occurs error !"                             
EOTS_BTOR      0x071D 0x8B "Block tolerance is out of range !"                               
EOTS_LSMS      0x071E 0x8C "LUN size does't match the setting !"                             
EOTS_S0HE      0x071F 0x8D "Spec.0 LUN size is small then 0x400 sectors !"                   
EOTS_S1HE      0x0720 0x8E "Spec.1 LUN size is small then 0x020 sectors !"                   
EOTS_TCLE      0x0721 0x8F "To create LUNs occur error !"                                    
EOTS_TFCE 0x98 0x0722      "To format and copy file occur error !"                      
EOTS_UVDE      0x0723 0x90 "Update vendor data occurs error !"                               
EOTS_SIFR      0x0724 0x91 "The size of ISP file is out of range !"                          
EOTS_SPND      0x0725 0x92 "The short page number is not define !"                           
EOTS_GIOE      0x0726 0x93 "Inquiry string is not match !"                                   
EOTS_CDIE      0x0727 0x94 "Get device information occurs error !"                           
EOTS_CDCE 0x12 0x0728      "Check device capacity occurs error !"                       
EOTS_VCIS 0x44 0x0729      "The bad block is too much !(valid capacity is too small)"                       
EOTS_CSNE      0x072A 0x95 "To create serial number occurs error !"                          
EOTS_CDUE      0x072B 0x96 "To create device occurs unknown error !"                         
EOTS_UDUE      0x072C 0x97 "To update device occurs unknown error !"                         
EOTS_RCTE      0x072D 0x99 "Running commands in thread occurs unknown error !"               
EOTS_ESBO      0x072E 0x9A "Erase block occurs error before creating %s table !"          
EOTS_EVBO      0x072F 0x9B "Erase VBs in WBT occurs error !"                                 
EOTS_SLOR 0x44 0x0730      "The bad block is too much !(start LBA offset is error)"                 
EOTS_FTOE      0x0731 0x9C "Flash testing occurs error !"                                    
EOTS_CUAP      0x0732 0x9D "%s LUN occurs error !"                                           
EOTS_DCIZ 0x12 0x0733      "The capacity of device is zero !"                           
EOTS_FSSE      0x0734 0x9E "The file system of %s is not correct !"                          
EOTS_FFSE      0x0735 0x9F "The file format of %s is not correct !"                          
EOTS_DCIS      0x0736 0xA0 "The capacity of device is too small !"                           
EOTS_WSRE      0x0737 0xA1 "To write system ready occurs error !"                            
EOTS_TCLS 0xA4 0x0738      "The capacity of \"%s\" is not enough !"                     
EOTS_CFIC 0x54 0x0739      "Can not find ISP code !"                                    
EOTS_PACM      0x073A 0xA2 "When page size is %s, channel must smaller than %s !"
EOTS_CLDE      0x073B 0xA5 "To create LED occurs error !"
EOTS_SINR      0x073C 0xA6 "System is not ready !"                     
EOTS_CPDE      0x073D 0xA7 "To create password occurs error !"         
EOTS_IBME      0x073E 0xA8 "Initial bad block management occurs error !"
EOTS_DSLF      0x073F 0xA9 "To disable security function occurs error !"
EOTS_BBTM      0x0740 0xAA "Bad block number is too much !"                     
EOTS_ECIM      0x0741 0xAB "Error code in system is not match !"                
EOTS_CNAA      0x0742 0xAC "Can not allocate \"%s\" address !"                  
EOTS_NFNE      0x0743 0xAD "To notify FW new system address occurs error !"     
EOTS_SBTF      0x0744 0xAE "In fixed cluster setting, the size must bigger than 2048MB !"
EOTS_GOLE      0x0745 0xAF "Get optimal setting of LUN occurs error !"
EOTS_RTCS      0x0746 0xB9 "Retry to create system occurs error !" 
EOTS_DCCV 0x44 0x0747      "The bad block is too much !(it is not contain VBSector)"
EOTS_DCHB 0x48 0x0748      "The capacity of device has been changed !"
EOTS_DDNA 0x44 0x0749      "The bad block is too much !(it is not contain AP LUN)"  
EOTS_IBIM      0x074A 0xBA "The bin type is not match !"        
EOTS_TRAE      0x074B 0xBB "To read AP lun occurs unknown error !"
EOTS_TFRA      0x074C 0xBC "The flash P/N can not operate on auto mode !"
EOTS_FFNM      0x074D 0xBD "The force flash P/N is not match !"
EOTS_CVIE      0x074E 0xBE "To clear VB in LUT occurs error !"   
EOTS_FDNQ      0x074F 0xBF "The force flash PN is not support for QC Item !"        
EOTS_RFOU      0x0750 0xC0 "Rebuild function occurs unknown error !"            
EOTS_GRTE      0x0751 0xC1 "Get rebuild table occurs error !"
EOTS_RBMC      0x0752 0xC2 "Rebuild function is not support for multi-channel !"   

EOTS_GALE      0x07B0 0xE0 "To get AP LUN data occurs error !"                             
EOTS_GCFE      0x07B1 0xE1 "To get content of Cfg. file occurs error !"                    
EOTS_RCFE      0x07B2 0xE2 "To read content of Cfg. file occurs error !"                   
EOTS_CDDE      0x07B3 0xE3 "To check device data occurs error !"                           
EOTS_GDIA      0x07B4 0xE4 "To get device info. in AP LUN occurs error !"
EOTS_CRTE      0x07B5 0xE5 "To check root table occurs error !"              
EOTS_CCIS      0x07B6 0xE6 "To check CIS table occurs error !"    
