If you want to update your BIOS, please execute the BAT file. Don't use AFUDOS directly.
When you execute the BAT file, it will automatic run the awdflash to update the new BIOS for your mainboard.(Note: Before update BIOS please make sure already disabled Flash Part Protect function in BIOS Setup)
The new BIOS was modified for the following reason:
    1. Improve discrete VGA card vBIOS compatiblity.

     
