KONICA MINOLTA magicolor 1650 PS/PCL Printer Driver
===================================================
Ver. 1.1.0

Common for PS/PCL driver
========================
- In the environment that printer drivers installed via "Point and Print" method, please edit "Favorite Setting" or "Watermark" in Printers folder, previously.

- If the font in the document is not printed as expected, try to change following options.
  [Quality] tab -> [Font Settings] -> change [Download Font Format] to Bitmap
  [Quality] tab -> [Font Settings] -> uncheck [Use Printer Fonts]

- Watermark may not be printed with a combination of the following functions.
  [Zoom], [N-up], [Binding Margin], [Grayscale]
To print the Watermark, change Watermark color from Black or Glayscale to Color and set Transparent to Off, or change the above setting.

- The [Remove White Background] setting in the [Other] tab will only function when using Microsoft PowerPoint 2003 or earlier. It will not function with PowerPoint 2007. The workaround for PowerPoint 2007 is to check "Hide background graphics" in "Format Background".

- Printing over WSD port from Windows Vista may result in an error page or only a partial job being printed. To prevent this, choose Raw port or LPR in the driver's [Properties] -> [Ports] tab.

- When printing certain complex PDF or Microsoft PowerPoint 2007 files, the printer may produce an error page or the job may continuously stop partway and then restart from the beginning. If this situation occurs, the workaround for PDFs is to check "Print as image" in the "Advanced Print Setup" section of the Acrobat or Acrobat Reader Print dialog box. The workaround for PowerPoint 2007 files is to check "High Quality" in the "PowerPoint Options" -> "Advanced" -> "Print" section. 

Notes for PS driver
===================
- "Booklet" may not be printed properly when "gradient" is selected for "fill color" with Microsoft Office applications. To print it properly, go to [Printing Preferences] -> [Advanced] tab and select "Disable" for [Postscript pass through].

- If the spool data exceeds few hundred mega bytes, it may cause a warning (insufficient memory) upon your system environment. To solve this problem, turn the following options disabled.
  [Printing Preferences] -> [Advanced] tab -> [Advanced Printing Features:]
  [Properties] -> [Advanced] tab -> [Enable advanced printing features]

- "Booklet" cannot be used with the following setting.
  Port: SMB or Internet Port
  [Printing Preferences] -> [Advanced] tab -> [Advanced Printing Features: Disabled]
  [Properties] -> [Advanced] tab -> [Enable advanced printing features: Not checked]

- In File Maker 4.0, please set the "Binding Position" from Printers folder.

- When printing with a pass through application such as Adobe Reader, the collate function in the Print dialog box may not function.
To use the collate function with pass through applications, either choose the PCL driver, or on the PostScript driver, choose the driver's [Properties] -> [Printing Preferences] ->  [Advanced] tab -> [PostScript Options] -> [PostScript Pass Through] -> [Disable].

- When printing with certain application such as Microsoft Word, Cover Page may not be added for each copy. To add Cover Page for each copy, use the PCL driver.

- When printing in the "Point & Print" environment, the Collate function in the Print dialog box may not function. To use the Collate function, install the driver locally on the client PC, or use the PCL driver.

- Watermark may not be printed when Grayscale is selected and reduced print or N-up. To print the watermark, in this setting please try one of these.
a. Select the other Quick Color option under the Quality tab
b. Select Custom in Quick Color, click the Details button, and select Smooth for the Halftone of Graphics.

Notes for PCL driver
====================
- In CorelDRAW application, it will take long time to print the document or cause "PCL XL error" if the pattern like gradation is used to fill the object. To solve this problem, please set CorelDRAW option as follows;
  [File] -> [Print] -> [Misc:]  Check "Rasterize entire page"

- In Microsoft Publisher, imported JPEG image may be printed upside down. To resolve this, please resize the image in another application prior to import into Publisher.

- Watermark, Cover Page, and Separator Page may not function when you use any 32bit application software on a 64 bit OS. To use these functions, check [EMF Spool] in the driver's [Properties] -> [Settings] tab.

Notes for Printer
====================
- When using Internet Explorer version 7, please add the correct path to the file within the Download Manager page or Direct Printing page on the PageScope Web Connection. Without the path, Internet Explorer will not send the file to the printer.

------------------------------------------------------------
Copyright(C) 2009 KONICA MINOLTA BUSINESS TECHNOLOGIES, INC.
All rights reserved.
